cript started on Tue Mar 24 10:40:41 1998


orca:/users/teto[31]> rlogin entropy -l pcdisk


Please wait...checking for disk quotas


        ***********************************************************





           ######  #    #   #####  #####    ####   #####    #   #


           #       ##   #     #    #    #  #    #  #    #    # #


           #####   # #  #     #    #    #  #    #  #    #     #


           #       #  # #     #    #####   #    #  #####      #


           


                    Welcome to HP-UX on the HP 9000 Series


                   Monterey Bay Aquarium Research Institute


                  HP-UX entropy A.09.04 E 9000/887 931751281





        ***********************************************************





[1] % cd /usr/troll


[3] % ./wf-seatel 


This is the program to connect to the seatel at the County Comm Site.


It is presently configured to talk to the Pt Lobos.


Elevation 085 seems to be the right number. That should be -1.5 degrees


Heading should be 312.5  (check with H set with B )


N040 Y000 X001 for defaults


Signal strength should be in the DXX range.


Type ESC Cntrl-B B to get to the Seatel.


Will auto timeout disconnect after 5 minutes.


ESC Cntrl-B D will get you a loopback at Toro


Connecting thru wf-seatel.port, speed 9600.


The escape character is CTRL-\ (28).


Type the escape character followed by C to get back,


or followed by ? to see other options.





[Back at Local System]


[4] % logout


Connection closed.


script done on Tue Mar 24 10:41:40 1998





