
MRC DATAQ MODEM SET-UP

S/N
AA041299
AA041300
AA041301
AA041302
AA041303
AA041304
AA041305
AA041306
AA041307
AA041308

T1:

ALARMS:
TX & RX RUN

000
TX & RX RUN

000
TX & RX RUN

000
TX & RX RUN

000
TX & RX RUN

000
TX & RX RUN

000
TX & RX RUN

000
TX & RX RUN

000
TX & RX RUN

000
TX & RX RUN

000

PASSWWORD
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A

AVERAGE PER
0E-8
0E-8
0E-8
0E-8
0E-8
0E-8
0E-8
0E-8
0E-8
0E-8

RX AIS ERRORS*
00000
00000
00000
00000
00000
00000
00000
00000
00000
00000

LCL CH# VOLTS
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A

RMT CH# VOLTS
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A

LCL ALARM SET UP
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A

CNTRL PT RELAY
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A

RMT PT RELAY
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A

RING STATION
SELECT
SELECT
SELECT
SELECT
SELECT
SELECT
SELECT
SELECT
SELECT
SELECT

RING ALL STNS
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A

OPERATE MODE
XMIT AND RECV
XMIT AND RECV
XMIT AND RECV
XMIT AND RECV
XMIT AND RECV
XMIT AND RECV
XMIT AND RECV
XMIT AND RECV
XMIT AND RECV
XMIT AND RECV

TX FREQUENCY
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz

RX FREQUENCY
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz
6.2 MHz

TX FRAME TYPE
PATTERN B
PATTERN B
PATTERN B
PATTERN B
PATTERN B
PATTERN B
PATTERN B
PATTERN B
PATTERN B
PATTERN B

RX FRAME TYPE
PATTERN B
PATTERN B
PATTERN B
PATTERN B
PATTERN B
PATTERN B
PATTERN B
PATTERN B
PATTERN B
PATTERN B

LINE CODE
B8ZS
B8ZS
B8ZS
B8ZS
B8ZS
B8ZS
B8ZS
B8ZS
B8ZS
B8ZS

STATION ID
  13
  02
  11
  01
30 (SPARE)
  14
  03
  12
  04
20 (SPARE)

REMOTE CONTROL
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A

CALIBRATION
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A

NEW PASSWORD
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A
N/A

LOCATION
SYS B TORO

6 GHz
SYS A TORO

18 GHz
SYS B MBARI
SYS A MBARI
SPARE
WESTERN FLYER
SYS A TORO

6 GHz
SYS B TORO

18 GHz
PT LOBOS
SPARE

*THIS SHOULD READ “00000” OR ANY NUMBER THAT IS NOT QUICKLY CHANGING.

