
Mt Toro 6 GHz frequency and filter switch

A - 
Operational configuration

1 - 
System A with have the RCVR channel set to CH 14, 6512.5 MHz, and the XMTR channel set to Ch 2,  6462.5 MHz. 

2 - 
System B with have the RCVR channel set to CH 11, 6437.5 MHz, and the XMTR channel set to CH 13, 6487.5 MHz.

3 - 
The channel filters are located in their respective radomes and are controlled by latching relays that are controlled from the equipment rack in the shelter. The control lines are included in the control cable to the respective Seatel pedestals.

    
System A uses pair # 14, W is the PL and BK is the WF. System B uses pair # 4, W is the PL and BK is the WF.

B - Changing configuration

DO NOT SWITCH THE RELAYS WITH TRANSMIT RF ENABLED!

1 - 
Insure that the respective antenna is pointed at the correct vessel.

2 - 
To change the configuration of either system, first place the transmit switch into "STAND-BY".  This will disable the transmit RF. Change the respective receiver and transmitter channel switches to their new positions. Go the the rear of the rack and momentarily apply +12 VDC to the  respective relay control wire. Go back to the  front of the rack and verify that the channel     

filters were switched to the new channel by looking at the monitor for clear video and at the receiver AGC, signal strength, to see that it is reading in the correct range. Now place the transmit switch back into "TRANSMIT".

