
2005M2 RADIO SWAP
Before you go to MT Toro to do the swap, perform the following in the OASIS lab and the Cupola.


MBARI CUPOLA FREEWAVE RADIO SWAP
1 - 
Depower and disconnect the Freewave radio in the OASIS lab.

2 -
Depower and disconnect the Bldg B Freewave link in the cupola

3 - 
Disconnect the DB25 at the back of the M2 modem. You will note that it goes to the M2 fiber converter.

4 – Cut the tiewraps and disconnect the DB9s between the Toro link Freewave radio and the Bldg B Freewave 
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      link. Connect the DB9 from the Toro link Freewave radio cable to the M2 fiber converter using the BSA 

     
sitting on the Freewave radio. Do not use the null adapter. Tiewrap for security.
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MT TORO MOORING RADIO SWAP

1 - 
Depower the Teledesign 2004M2 radio and remove the antenna, blue color code. 

2 - 
Depower the Teledesign 2005M2 radio and remove the antenna. Install the antenna, blue color code, on the 

     Teledesign 2005M2 radio and apply power. 

3 - 
Install the antenna that was on the Teledesign 2005M2 radio on the back of the monitor radio and apply 

     
power.

4 - 
Call Kent and have him try to contact the mooring while watching the activity LEDs on the Freewave and 

     
Teledesign radios. On the Freewave, the green link LED should be illuminated and the TX LED should be 

     
flashing while on the Teledesign the TX LED should be flashing, this is in response to the keystrokes by Kent.
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