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UHF TELEDESIGN RADIO TRAVELER

RADIO
TS4000A05B45SN

S/N
17012 - SMA


SPEC
MEAS
DATE
                      COMMENTS

FREQ 1
461.7625
461.7629
28APR05
CLEAR CHAN SCAN – TWO FREQS

FREQ 2
461.7875
461.7879
28APR05
FIRMWARE: REV: 4.64  BOARD: REV: 1.02 

S/N: 17021

PO
5W
5W
28APR05
RADIO TYPE: 3412  S/N: 30490

ITX
<2.20A

@12.5VDC
1.82 A

@12.5VDC
28APR05


DEV
±3 KHz
±3 KHz
28APR05


RSENS
>-105 dBm
-110 dBm
28APR05


IRX
<200 ma

@12.5VDC
180 ma

@12.5VDC
28APR05


BENCH TEST
PASS
28APR05


    CAN #
N/A



  MOORING




IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



 FINAL SOFTWARE CONN WITH 

 “TORO”



IN BAR

1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



 FINAL SOFTWARE CONN WITH 

 “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN WITH “TORO”



 FINAL SOFTWARE CONN WITH   

 “TORO”
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