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UHF TELEDESIGN RADIO TRAVELER

RADIO
TS4000A05B45SN

S/N
18352 - N


SPEC
MEAS
DATE
                      COMMENTS

FREQ 1
466.7625
466.7629
3OCT05


FREQ 2
466.7875
466.7879


3OCT05


PO
5W
5W


3OCT05


ITX
<2.20A

@12.5VDC
1.72A

@12.5VDC
3OCT05


DEV
±3 KHz
±3 KHz


3OCT05


RSENS
>-105 dBm
-110 dBm


3OCT05


IRX
<200 ma

@12.5VDC
175 ma

@12.5VDC
3OCT05


BENCH TEST
PASS
3OCT05


    CAN #
N/A



  LOCATION


MT TORO

IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



 FINAL SOFTWARE CONN WITH 

 “TORO”



IN BAR

1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



 FINAL SOFTWARE CONN WITH 

 “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN WITH “TORO”



 FINAL SOFTWARE CONN WITH   

 “TORO”



ACCEPTANCE BY MOORING MASTER

NAME: 

TITLE: 

DATE: 
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