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UHF TELEDESIGN RADIO TRAVELER

RADIO
TS4000A05B45SS

S/N
22849 - SMA


SPEC
MEAS
DATE
                      COMMENTS

FREQ 
466.4000
466.40006
20OCT04
RADIO TYPE: 3412  S/N: 37669

PO
2.5W
2.5W
20OCT04
FIRMWARE: rev4.76  BOARD: rev1.06 S/N: 22849

ITX
<1.60A
1.29 A
20OCT04


DEV
±3 KHz
±3 KHz
20OCT04


RSENS
>-105 dBm
-110 dBm
20OCT04


IRX
<200 ma
167 ma
20OCT04


BENCH TEST
PASS
20OCT04


    CAN #
N/A



  MOORING




IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



IN BAR

1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”
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