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Board Serial Number:____________________   Board Revision Number:____________________





Date_____________ Engineer ____________________ Technician __________________________





Application for this configuration _____________________________________________________





Motor Power Supply:    Voltage____________  Current (peak) ____________





Module Power Supply:   Voltage___________   Source,  J1  jump W2 1-2   <or>   J3 jump W2 2-3





Local Regulation:    Yes,  W1 1-2  and   W3 2-3   <or>    No,  W1 open and W3 1-2





PWM input:     Active Hi   W4 1-2    <or>   Active Lo  W4 2-3





Direction Input:   “A” output follows input, W5 1-2   <or>  “B” output follows input, W5 2-3





Feedback Pot configuration:   2 wire W6 2-3, W7 2-3  <or>  3 wire W6 1-2, W7 1-2





Feedback amp non standard comp values..?  R27_______  R29______  R30______ R31______





TP2 output: ________________ Volts at ________________ Ohms





Overcurrent detector setup:  Gain at TP3______Amps/Volt   R28______  R3______ R4______ 





Overcurrent detector time constant: ______________  R17_______  C4________





Set Overcurrent trip to: ____________________ Amps





Filtered current output:  Gain at TP4_______Amps/Volt   Rolloff (3db)_________Hz 





                                            R24__________   R25_________    C9_________





Transient Supressor  D4: _______________Volts,  Part Number_________________





Connector types:   J1__________________________   J2__________________________





J3_______________________  J4_______________________  J5________________________





Notes: ____________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________





END


          


�PAGE  �2�








�PAGE  �2�

















