ELECTRICAL TEST CERTIFICATE

	Product:
	RM0011
	Client:
	MBARI
	P/O No:
	TBC

	
	
	W/O No:
	9879

	Length(s):
	
	Certificate No:
	9003


	ROUTINE TESTS

	Component
	Conductor Resistance

((/km max. @ 20°C)
	Insulation Resistance

(M(.km min. @ voltage specified)

	
	
	Core / Core
	Core / Screen
	Screen / Screen

	0.22 mm² STQ (x 1):
	88.0
	1,000 @ 1.0 kVdc
	1,000 @ 1.0 kVdc
	- - - -

	STQ screen:
	Test continuity (measure & record CR).
	- - - -
	- - - -

	4.0 mm² (x 5):
	4.8
	1,000 @ 5.0 kVdc
	1,000 @ 5.0 kVdc
	- - - -

	Collective screen:
	Test continuity (measure & record CR).
	- - - -
	- - - -


	ADDITIONAL TESTS

	Component
	Test Description
	Test Parameter(s)

	SM fibre optic (x 5):
	Attenuation @ 1,310 nm.
	0.45 dB/km max.

	
	Attenuation @ 1,550 nm.
	0.35 dB/km max.

	MM fibre optic (x 1):
	Attenuation @ 850 nm.
	3.5 dB/km max.

	
	Attenuation @ 1,300 nm.
	1.5 dB/km max.


We certify that the product(s) detailed hereon have been inspected and tested / conform in all respects with Cortland Fibron BX Ltd specification(s) and, unless otherwise stated, conform in all respects with the requirements of the contract or order.



