Power Cable Consultants, Inc.


Review of Cortland Drawing SQ16512 (rev02), dated 13/10/10
The proposed design has several electrical improvements compared to the existing umbilical cable construction.

Below find PCC’s questions to clarify the composition of some of the components in the final design.
A, the screened quad:  

In Option 3 this item was jacketed with XLPE.  Will it be jacketed in the Final Design?
B, the stainless steel tube with fiber optics:
Will the tube be jacketed and will the material be XLPE?
C, the power conductors:
Will the insulation thickness be 0.58 mm and will the material be XLPE?
Assembly Voids:
Will the assembly voids be filled with silicone rubber compound?
Other Items:
Will the cable core be jacketed with high density polyethylene material (0.8 mm nominal thickness)?
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