10020865rB Four Channel Serial/Power Mux
Board rework directions:

MUXER 5V TO 3.3V Low Power Operation Modification:
1) REPLACE K1, K2 AND K3 DSP2A-L2-DC5V relays with DSP2a-L2-DC3V relays
2) REPLACE U14 LT1129CST-5 with LT1129CST-3.3

MUXER External POR Circuit for U3 Modification:
1) REMOVE J8
2) INSTALL PIN2 OF DS1818-10+ INTO J8.3
3) INSTALL PIN3 OF DS1818-10+ INTO J8.4
4) JUMPER PIN1 OF DS1818-10+ OVER TO SIDE OF R32 THAT MAKES CONNECTION WITH
PIN3 OF U3

MUXER Sample Resistor Change:
1) REPLACE R36 SR10-0.01 with SR10-0.10

MUXER R37 and R38 Change:
1) USE ZERO OHM VALUE

MUXER R23 Change:
1) USE 22AWG Bus Wire with Teflon sheathing

MUXER JP3,4,5,6 Strapping Configuration:
1) JUMPER PINS 2 & 3 FOR JP3, JP4, JP5 and JP6
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