LRAUV Load Control Low-Voltage Converter
MBARI 11021173
Design Notes

2015 Sep 1	ecm	init

Requirements

1)	

Approach

Design Notes

1.	LTSpice sim of start-up to establish Soft Start timing vs. cap load. 
Initial SS cap (from LT download) is 1 nF; charges to ~1V in 0.5 ms.