ESP SYRINGE REV1-0 SPECIFICATION READ-ME
File Name:  ESPSYRINGE_REV1-0.MAX
Layers: 2 

Layer Orientation:


1: TOP


2: GND
Thickness:  0.031 "" FR4 

Dimensions: 1.0” x 0.85" 

Final Thickness: 0.031”

Finish: SMOBC / HASL
Cu Weight: 1oz (TOP,BOT)
Trace width/space: 0.0010”/0.007”
Smallest hole size: 0.030" 

Sides to solder mask: Both Sides (BLACK)

Sides to silk screen:  Both Sides (WHITE) 

NO TEST REQUIRED…
