TETHYS SERIAL TEST BOARD SPECIFICATION READ-ME
File Name:  10020131_TETHYS-SERIAL-TB.brd
QTY: 10 MIN
Turn Time: 4 Days 

Layers: 4 

Layer Orientation:

1. TOP

2. GND

3. PWR

4. BOT

Thickness:  0.062 "" FR4 

Dimensions: 3.45” x 4.95" 

Finish: SMOBC/HASL 

Cu Weight: 1oz (ALL LAYERS)
Trace width/space: 0.005”/0.007”
Smallest hole size: 0.010" 

Sides to solder mask: Both Sides (BLACK)

Sides to silk screen:  Both Sides (WHITE) 

IPC-356 FILE (10020131_TETHYS-SERIAL-TB.ipc) INCLUDED FOR TEST
