Files to send out to fab…
1. Gerbers

a. Top copper (Keep artwork settings default unless otherwise specified)

b. Bottom Copper (Keep artwork settings default unless otherwise specified)

c. Inner copper (Keep artwork settings default unless otherwise specified)

d. Silk screen

i. Silkscreen Top

1. Board Geometery

a. Outline

b. Silkscreen_Top

2. Package Geometery

a. Silkscreen_Top

3. Components

a. RefDes – Silkscreen_Top

ii. Silkscreen Bottom

1. Board Geometery

a. Outline

b. Silkscreen_Bottom

2. Package Geometery

a. Silkscreen_Bottom

3. Components

a. RefDes – Silkscreen_Bottom

e. Soldermask

i. Soldermask Top

1. Stack-up

a. All – Soldermask_Top

2. Board Geometery

a. Soldermask_Top

3. Package Geometery

a. Soldermask_Top

ii. Soldermask Bottom

1. Stack-up

a. All – Soldermask_Bottom

2. Board Geometery

a. Soldermask_Bottom

3. Package Geometery

a. Soldermask_Bottom

f. Pastemask

i. Pastemask Top

1. Stack-up

a. All – Pastemask_Top

2. Package Geometery

a. Pastemask_Top

ii. Pastemask Bottom

1. Stack-up

a. All – Pastemask_Bottom

2. Package Geometery

a. Pastemask_Bottom

g. NC_Drill file

h. IPC-356 Netlist for error checking

2. Drawings

a. Drill/Manufacturing drawing

i. Dimensions

ii. Board outline

iii. Drill chart

iv. Fabrication notes

v. Sheet information

b. Assembly drawings

i. Top

ii. Bottom

c. Schematic PDF

d. BOM PDF

