ESP 1020877rA PWM Test Procedure
Technician:__________________________
Date:_______________________________
1. Set power supply to 10V.

2. Set current meter to 1V/A

3. Set scope to the following:

a. 500mV/div

b. 500mS/div

c. Single edge trigger.

i. Rising edge.

d. Probe set to 1X

4. Record the time it takes to go from full current to constant current state.

5. Set scope to Run.

a. 100mV/div

6. Record current draw at 10V.

7. Apply test voltages 12V, 14V, and 16V to circuit board and record current during constant current state.
	SN\Voltage
	10V

(mA)
	12V

(mA)
	14V

(mA)
	16V

(mA)
	Transition (s) 

	ESP001
	
	
	
	
	

	ESP002
	
	
	
	
	

	ESP003
	
	
	
	
	

	ESP004
	
	
	
	
	

	ESP005
	
	
	
	
	

	ESP006
	
	
	
	
	

	ESP007
	
	
	
	
	

	ESP008
	
	
	
	
	

	ESP009
	
	
	
	
	

	ESP010
	
	
	
	
	


Notes:
