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Thursday, December 06, 2012


Cable Type Falmat FM022208-11-M02


AWG 14 Conductor equivalent is 4 x #20AWG


Waterblocking (Cable Max?) present


Twists on twp should be  maintained to solder cups as best as


possible.


Jacket:Green Polyurethane


Dia: 0.61"
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1 Power +


2 Bi-directional pair A+  Twp #1 (grn)


3 Bi-directional pair A-  Twp #1 (wht)


4 Bi-directional pair B+  Twp #2 (org)


5 Bi-directional pair B-  Twp #2 (wht)


6 Bi-directional pair C+  Twp #3 (brn)


7 Bi-directional pair C-  Twp #3 (wht)


8 Bi-directional pair D+  Twp #4 (blu)


9 Bi-directional pair D-  Twp #4 (wht)


10 Power –


#20 AWG Brown


VAC Line/DC+


VAC Neutral/DC-
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