901112 - MBTS; Android data logger : Procedure for drifter deployment This page last changed on Apr 17, 2013 by oreilly. Connect phone to IOIO board with USB Plug cable from battery pack to Wakey; verify that SPOT and IOIO power LEDs are now lit NOTE: to power-cycle Wakey, unplug the power cable for at least 30 seconds before re-plugging Run "IOIO Hardware Tester" app, verify comms with IOIO board If no comms with IOIO: Verify IOIO board has power from Wakey Reboot phone Turn off unneeded phone radios: Turn off GPS Put phone in 'Airplane mode' Enable Bluetooth Run Drifter app Run Diagnostics -> Wakey test (puts Wakey to sleep) Run Diagnostics -> SPOT test Run Manual Refresh Before stowing phone in housing, consider dimming phone screen to save power (the screen will light on each sample cycle while IOIO has power)

Document generated by Confluence on Feb 03, 2026 15:53