CANON Data : Autonomous Vehicles Working Group This page last changed on Aug 27, 2013 by mjstanway. ## Dorado ## Gliders ## Long-Range AUVs (LRAUVs) ### Tethys Tethys will circle the Northern ESP, then run a lap around a box oriented East-West. The Western edge of the box is currently adaptive at the user level (single command to change the longitude), with plans to make it adapt autonomously by detecting a front using Yanwu's algorithm, as time permits. ### Daphne Daphne will circle a submerged LST, using the Benthos DAT to query an acoustic modem on the LST roughly once every minute. ## Lagrangian Sediment Traps (LSTs) Operating depth 100 m Two-day deployments ##### Attachments There are currently no attachments on this page.

Document generated by Confluence on Feb 04, 2026 08:09