SAMPLES WORKING GROUP
1. Operational definition of sample: A physically-collected sample, as distinct from an electronically-collected datum. 
2. Purpose: 

· Provide some coordination for the taking of samples by the different platforms and research groups --- goal of insuring complete datasets are obtained

· Budget water and effort

· Document responsibilites

· Document sample collection, processing and data flow
· Interface with Data Management and Analysis
3. Platforms and routine samples:

· CTD rosette Niskin bottles:



-Depths: 0,0, 5, 10, 20, 30, 40, 60, 80, 100, 150, 200m



-Profiles: Macronuts, ammonium, chl, C14-PP, ?triplepoint-PP


-Surface: POC, HPLC, FCM, A*, QP, 5&1um Chl and C14-PP
-Additional: Winkler oxygen, salt, DIC/TCO2, ALK, N03&NH4-PP
· Profiling pumped CTD
-???
· AUV Gulpers

-???
· ESP

-???
· Drifting sediment traps

-???

· Drifting productivity arrays

-0, 5, 10, 20, 30, 40m

-C14-PP, NO3&NH4PP, O2-PP, final macronuts and NH4, POC, QP
· Other …

