901303 Cytometer Technologies for Autonomous Platforms : Digital holographic microscopy This page last changed on Feb 03, 2014 by oreilly. Digital holographic microscopy at Wikipedia The LISST Holo has been integrated with Dorado Jericho et al describe a submersible digital inline holographic microscope (SDIHM), with ~2 micron spatial resolution and subsecond temporal resolution. Rated to 20 meters depth. A deep version rated to 6000 meters, with ~5 micron resolution is described by Bochdansky et al. Spatial resolution is considerably higher than LISST Holo (~25 microns). Video presentation; describes lightweight 2 kg version for arctic app. A version of this instrument is sold by Resolution Optics. Simplicity: microscopy without lenses; laser + pinhole + CCD camera Maximum information: single hologram contains all 3D structural information Maximum resolution: "optimal" resolution "easily" attainable - down to level of bacteria Speed kinetics of motion/reactions can be followed at video rate in 3D Resolution Optics might lend a Submersible Microscope to MBARI for evaluation. Attachments: SubmersibleHolographicMicroscope.pdf (application/x-pdf) DeepDIHM.pdf (application/x-pdf)

Document generated by Confluence on Feb 03, 2026 16:08