901303 Cytometer Technologies for Autonomous Platforms : Technologies overview - 3 (Specifications and parameters)) This page last changed on Jul 11, 2013 by klimov. Variables and parameters
Parameter | Notes | Range |
--- | --- | --- | ---
Cell size range, um - detectable - filtration |  |  |
Concentration range, cells/mL |  |  |
Detection volume, uL, mL |  |  |
Flow rate, mL/min, uL/min - per channel cross section - per detection cross-section |  |  |
Throughput range, counts/sec. 2E5 (LLNL) |  |  |
Signal processing speed (pulses/sec, images/sec) |  |  |
Overall energy efficiency; J/count |  |  |
Statistics and acceptable errors |  |  |
Optical background (Br) |  |  |
Detector efficiency (Qr) - determined by laser power, optical design, PMT sensitivity... photoelectrons detected per equivalent fluorochrome molecule |  |  |
Linear range (signal : number of photons) |  |  |

Document generated by Confluence on Feb 03, 2026 16:08