900731 Data Handling for Eye-in-the-Sea on MARS : EITS This page last changed on May 11, 2011 by dcline. # EITS ## About EITS EITS is a really boring name for the Eye-In-The-Sea computer that hosts a large RAID to store raw and processed data. It is also responsible for sending off jobs to execute the EITS workflow. EITS is a HP xw4400 Workstation running Windows Server Enterprise SP2. ## MARS Network Settings
IP | 134.89.12.144
Submask | 255.255.254.0
Gateway | 134.89.12.1
DNS 1 | 134.89.12.87
DNS 2 | 134.89.10.32
## Add-on hardware A Host bus adapter (HBA) card was installed to interface to the RAID. This is a LSI Logic LSISAS344SE-R PCI Express to 3.0 GB/s Serial Attached SCSI (SAS) Host Bus Adapter. ## Add-on software LSISAS344SE-R PCI driver (available for download from LSI logic site) NStor host-based version on shipped CD. Insert CD, and once autoplay starts, navigate to E5412E->Install StorView (Host Based). cygwin http://www.cygwin.com/; Select the following additional non-default packages to install: rsync, vi, emacs, bash, cygrunsrv, perl, subversion, openssh, xterm, and cvsutils. JDK 6 Update 4 from http://java.sun.com/javase/downloads/index.jsp ## Experiment software EITS workflow scripts and cron job installation EITS web service EITS RAID directories EITS cron setup EITS rsync setup EITS streaming setup Attachments: cygwin.jpg (image/pjpeg) administrative.jpg (image/pjpeg) startrsyncd.jpg (image/pjpeg) startrsyncd.jpg (image/pjpeg) rsync.jpg (image/jpeg) cron.jpg (image/jpeg)

Document generated by Confluence on Feb 03, 2026 14:51