900719_FOCE : XFOCE - Phytec LPC3250 Evaluation This page last changed on Sep 11, 2012 by headley. # Evaluating Phytec LPC3250 as Gateway Node Hardware Candidate ### LPC3250 Specs/Features
Processor | NXP LPC3250
Instruction length | 32 bit
Clock frequency (MHz) | 208 MHz
Memory On-chip | 32 KB L1, 256 KB SRAM
DRAM | 16/32/64/128 MB LPSDR
NAND | 16/32/64/128 MB
NOR | 1/2/4/8 MB
FLASH |
EEPROM | 32K
Floating Point | VFP
Input Voltage | 3.15 V
Programmer HW | ?
Programmer SW | ?
Bootloader | ?
PCB | 58 x 70 mm
weight | ?
Debug Support | JTAG+?
Expansion Connectors | ?
Micro SD Card/SDIO/MMC | 2
USB | Host // OTG 1 FS
UART | 7
RS232 | 2
Ethernet | 10/100
SPI/SSP | 4
I2C | 2
I2S | 2
CAN | N
Digital IO |
ADC | 3x10 bit
DAC | ?
PWM | Y
Timers | ?
Watchdog | ?
RTC | N
vendor | Phytec
form factor | 58 x 70 mm
cost | USD $500
features | ?
Build Environment | ELDK, LTIB
C, C++ | Y
Java | oracle SE embedded+?
Language support | C, C++, Java + ?
Peripheral libraries | ?
OS support | LPC Linux
debugger | ?
IDE | ?
Command line | ?
User Support | phytec, forum?, web
### Out of the box What's in the box ### Toolchain, Environment VMWare Ubuntu Virtual Disk (SD Card) ELDK, LTIB tftp, S1 boot loader, u-boot ### Configuration, Packages #### Java VMs ##### Oracle SE Embedded #### Java Environment JAVA_HOME gnu.io.rxtx.SerialPorts #### RXTX #### LCM #### zeroMQ ### Building Build pre-defined image Customize image build add packages configure kernel Create disk image Partition and format microSD/mmc card Install disk image to SD Card ### Resources LPC3250 product page http://www.phytec.com/products/som/ARM-XScale/phyCORE-ARM9-LPC3250.html LPC3250 user manual http://www.phytec.com/pdf/manuals/ARM9/LPC3250/lpc3250.01_user_manual.pdf LPC3250 data sheet http://www.phytec.com/pdf/datasheets/ARM9/LPC3250/lpc3220.lpc3230.lpc3240.lpc3250.pdf LPC Linux Site http://www.lpclinux.com/ NXP BSP page http://ics.nxp.com/support/software/lpc32xx.bsp.linux/

Document generated by Confluence on Feb 03, 2026 14:29