900719_FOCE : Running FOCE in Test Tank This page last changed on Nov 13, 2008 by bobh. You must use the white Netgear router to emulate MARS. See Network Setup for MARS and Setting up Netgear Router The router is configured with a Building B address (134.89.12). This doesn't work outside building B without changing the router's WAN address The Netgear router is set up for address 134.89.12.162, which is a static Building B address that has a DNS name of focetest1 So, once you've connected the FOCE frame to the Netgear router, you simply need to ssh to ops@focetest1. Everything should work from there. Note - the Digi software on the FOCE laptop is set up to talk to the numeric address of 134.89.12.162. If you change the router WAN address, you'll need to change the Digi software on the laptop. See the "Serial Ports" section of Setting up Netgear Router.

Document generated by Confluence on Feb 03, 2026 14:29