900719_FOCE : xFOCE - Phytec LPC3250 - Configuration This page last changed on Aug 16, 2012 by headley. ###### ELDK does build uboot ../lpc32x0/uboot/u-boot-2009.03/uboot.bin kernel (uImage) in ../lpc32x0/kernel/linux-2.6.34/arch/arm/boot/ ###### ELDK does not build rootfs.jffs2. Includes default ramdisk rootfs in arm/images/uRamdisk, ramdisk_image.gz ###### LTIB builds kernel () in ltib/rpm/BUILD/linux-2.6.34/arch/arm/boot/ rootfs (rootfs.jffs2) in ltib/ ###### Jumper Settings for SD Card Detection [ref PHYTEC LPC3250_HM.pdf manual, sec 16.13] JP6: 2+3 (perm power SD card IF) [tethys uses 1+2] JP36: CLOSED (Enable SD card detect) [tethys uses OPEN ###### Other relevant jumpersL=: JP35:CLOSED JP37:CLOSED (write protection disable?) [tethys uses OPEN]

Document generated by Confluence on Feb 03, 2026 14:29