900719_FOCE : Workhorse Monitor ADCP This page last changed on May 31, 2008 by ckecy. # General Description The Monitor is Teledyne RD Instruments' most popular direct-reading Acoustic Doppler Current Profiler (ADCP). The unit is typically bottom frame-mounted and hard-wired to shore to provide real-time monitoring of coastal currents. The Monitor's high data accuracy and reliability make it a favorite for deployments in high volume traffic areas such as ports and harbors, where the data is often integrated into a Vessel Traffic Monitoring System. In fact, the Monitor has been selected for most major port programs undertaken in the United States. The Monitor offers a choice of three frequencies and ranges, to meet a wide array of data requirements. The unit also offers a flexible upgrade path, which includes an external battery pack, pressure sensor, bottom tracking capability for moving boat applications, and directional wave measurement. # Links Datasheet Setup Guide User's Guide Technical Manual Software Manual RDI Instruments Home Page Attachments: web_monitor1105.jpg (image/pjpeg)

Document generated by Confluence on Feb 03, 2026 14:29