900719_FOCE : FOCE Serial Expander This page last changed on May 28, 2008 by ckecy. # General Description Connect Tech's Xtreme/104-Plus family combines the best of the Universal PCI bus with the rugged and compact form factor of PC/104. PCI 2.0 and PC/104-Plus 2.0 compliant, the modular Xtreme/104-Plus and Xtreme/104-Plus Opto cards include a PC/104 pass-through connector option for compatibility with legacy PC/104 cards. Xtreme/104-Plus and Xtreme/104-Plus Opto offer independent port configuration for baud rate, and data bit options of 5, 6, 7 and 8 as well as 1, 1.5 and 2 stop bits. Select between odd and even parity. Connect Tech's Xtreme/104-Plus cards are perfect for embedded applications such as industrial PCs, kiosks, military systems, aerospace, medical systems, POS devices and any system requiring fast data transfer speeds and a rugged, compact form factor. These self-stacking cards are low on power consumption and function in industrial temperature conditions. # Links Datasheet Manual ConnectTech Home Page # Features Universal PC/104-Plus adapter PCI 2.0 and PC/104-Plus compliant 2 port model: 2 ports RS-423 4 port models: 4 ports RS-423 or 4 ports jumper selectable RS-232/422/485 8 port models: 8 ports jumper selectable RS-232/422/485 8 ports jumper selectable RS-232/422/485/TTL model Supports full duplex, half duplex and multi-drop communication modes in RS-422/485 (full duplex only in TTL model) TTL model has the ability to disable ports when not in use Maximum data speeds of 115.2 Kbps (RS-423), 921.6 Kbps (RS-232/TTL) and 1.843 Mbps (RS-422/485) Operating temperature range of -40ºC to 85ºC, storage temperature of -40ºC to 185ºC Each port can be configured independently for baud rate, parity, data and stop bits High performance PCI UARTs PC/104 pass-through connectors installed for compatibility with legacy PC/104 cards on select models Software support for Windows NT/CE/2000/Server 2003/XP/XPe/XPx64/Vista, Ardence RTX for Windows QNX 4/6, Linux and SCO Unix/Openserver. Multilayer PCB built with EMI reduction techniques Built with low power CMOS components PCI plug and play -- no jumpers to set for memory or interrupt configuration # Connector Locations # FOCE Serial Port Assignments The Xtreme104-Plus has eight serial ports. The following table displays the port assignments and associated communications parameters.
Port # | Type | Device Name | Device | Location
--- | --- | --- | --- | ---
1 | RS-232 | ttyS4 | SBE52 CTD #1 | pH Chamber
2 | RS-232 | ttyS5 | Vector ADV | pH Chamber
3 | RS-232 | ttyS6 | OceanLED | pH Chamber
4 | RS-232 | ttyS7 | Expansion Port | pH Chamber
5 | RS-232 | ttyS8 | SBE52 CTD #2 | Reference Instruments
6 | RS-232 | ttyS9 | Sunburst SAMI | Reference Instruments
7 | RS-232 | ttyS10 | RDI ADCP | Reference Instruments
8 | RS-485 | ttyS11 | Motor Controllers #1 and #2 | Arm A and B
Attachments: XP003_8web.jpg (image/pjpeg) Xtreme104 Conn Loc.JPG (image/pjpeg)

Document generated by Confluence on Feb 03, 2026 14:29