900719_FOCE : FOCE Computer Power Supply This page last changed on Apr 18, 2008 by chadillac. # General Description The HE104+DX is a high efficiency, high performance DC-to-DC converter that supplies +3.3V, +5V, +12V & -12V outputs to the PC/104 and the PCI-104 bus (also known as the Plus connector on the PC/104+ format). The HE104+DX is designed for low noise embedded computer systems, has a wide input range of 6-40V(>6:1) and is ideal for battery or unregulated input applications. The HE104+DX is specifically designed for vehicular applications and has heavy-duty transient suppressors (9000W on both main and secondary inputs) that clamp the input voltage to safe levels, while maintaining normal power supply operation. The HE104+DX is a state-of-the-art Mosfet based design that provides outstanding line and load regulation with efficiencies up to 90 percent. Organic Semiconductor Capacitors provide filtering that reduces ripple noises below 20mV. The low noise design makes the HE104+DX ideal for use aboard aircraft or military applications or wherever EMI or RFI must be minimized. The +5VDC and +12VDC outputs are controlled by a constant frequency architecture regulator that provides excellent line and load transient response. The HE104+DX has an opto-coupled on/off input (SD) to control the outputs of the HE104+DX. To enable the HE104+DX outputs, a 6 to 40V signal must be connected to the SD input. If remote control is not required, the SD input can be connected to the main power input. The common for the remote 6 to 40V signal must be connected to the HE104+DX common. If the SD input is connected directly to the main input power connector, the common for the SD input is already done. # Specifications
Parameter | Values
5V Output | 15A
12V Output | 3A
3.3V Output | 10A
-12V Output | 0.5A
Input Voltage Range | 6 to 40V
Load Regulation (5V) | <60mV
Line Regulation | 40mV
Output Temp. Drift (5V) | <40mV
Switching Freq. | 75kHz
Max. Input Transient | 125V for 100msec
Output Ripple (5V) | <20mV
Conducted Susceptibility (5V) | >57dB
Efficiency (5V) | Up to 90%
Temperature Range | -40 to +85C
Size | 3.55"W x 3.75"L x 0.6"H
# Connector Locations # Links Datasheet User's Manual Attachments: he104_plus_dx.gif (image/gif) HE104_plus_dx_conn_loc.JPG (image/pjpeg)

Document generated by Confluence on Feb 03, 2026 14:29