900719_FOCE : xFOCE - Phytec LPC3250 - Install ELDK Linux Build Tools This page last changed on Aug 16, 2012 by headley. ELDK is an alternative to ELDK for configuring Linux kernels for Phytec. ELDK is used to generate the kernel (uImage), though you have to generate u-boot (u-boot.bin) and rootfs (rootfs.tgz) images using other tools (e.g. LTIB, which is older, but simple and generates everything you need). =================== Install ELDK =================== - create directory structure: • /home/user/projects/eldk42 • /home/user/projects/lpc32x0 • /home/user/projects/lpc32x0/uboot • /home/user/projects/lpc32x0/kernel • /home/user/projects/lpc32x0/temp_dir • /home/user/projects/lpc32x0/downloads - follow instructions here http://www.lpclinux.com/LPC32xx/LPC32x0GettingstartedELDK - use Firefox or other browser in Ubuntu to download ELDK iso image - move ELDK iso to projects - mount the iso image $ cd projects/lpc32x0 $ mkdir temp_dir $ sudo mount -o loop downloads/arm-2008-11-24.iso temp_dir - run install script () - run (as root) ELDK_FIXOWNER - (see ftp://ftp.denx.de/pub/eldk/4.2/arm-linux-x86/distribution/README.html#Section_1.6.) - user@ubuntu:~/projects/eldk42$ sudo ../lpc32x0/temp_dir/ELDK_FIXOWNER -a arm - takes a couple of minutes ===================

Document generated by Confluence on Feb 03, 2026 14:29