Support Engineering Group : Shark Cafe Camera This page last changed on Mar 05, 2015 by tm. 2015 Tasks Housing polycarbonate tube (tough) Camera dimension un-housed is 1.11" at the back. tail section with pressure sensor and antenna hole - potted acrylic camera dome Fin clamp holder separate battery housing - detaches on release syntactic foam prop speed coating Camera RelayXD PrimeX Need to measure low light sensitivity Camera Controller Camera interface board Energy Harvesting board with WiPo Power input board Remote control/status board Processor board AT328 running at 4.5uA Solar Alta Devices flex Sensors and Satellite radio SeaTag MOD board Software behavior detect alg in SeaTag MOD SeaTag MOD on LRAUV to gather test data

Document generated by Confluence on Feb 03, 2026 16:22