Support Engineering Group : HRpH Sensors for Apr 2011 Deployment This page last changed on Mar 31, 2011 by tm. FOCE deployment planned for Apr 4, 2011. Delayed due to valve controller integration challenges on C02 enriched seawater box. Planned for first week of May 2011. 9 HRpH sensors were built - 6 optimized range for the FOCE frame (4 inside, 2 outside) and 1 full range for the ESW box. Preliminary assignments: pH1 1724 180358A - Optimized, 3.5 - 11.5, Range HRpH pH2 1735 180512A - Optimized, 3.5 - 11.5, Range HRpH pH3 1722 180513A - Optimized, 3.5 - 11.5, Range HRpH pH4 1749 180506A - Optimized, 3.5 - 11.5, Range HRpH pH5 1734 180511A - Optimized, 3.5 - 11.5, Range HRpH pH6 1751 180508A - Optimized, 3.5 - 11.5, Range HRpH ESW (pH7) 1753 180346A - Full, 0 - 14, Range HRpH Spare1 1723 180451A - Optimized, 3.5 - 11.5, Range HRpH Spare2 1790 180465A - Full, 0 - 14, Range Calibration Spreadsheet Attachments: HRpH_Cal110331.xls (application/vnd.ms-excel)

Document generated by Confluence on Feb 03, 2026 16:22