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Elevator Release Procedure
This process assumes Fusion USBL software is in running and you can track the beacon.  You also must know what address the beacon was programmed with.  This address can only be read and set with the Sonardyne beacon software. 
1. Select “Tools” tab > Manual Commands
2. Select beacon (i.e. elevator)

3. Enter “Cfg” for beacon

4. Select “Commands” tab

5. Choose “Enable” button : Sending enable command popup window should appear
6. Enter “RL” in send window

7. Initiate “Send” with send button : Sending command “RL” popup window should appear

8. In response window you should see release count X displayed. 

If you’re unable to get communications with beacon, adjust transmit & receiver gains in “Transceiver USBL 1 Properties. 
