STEDS Transmitter setup
· Current STEDS uses a Wildlife Computers PAT Mk10 device that is able to log depth, temp against time and features a conductivity switch to detect when the float is on the surface, whereupon it begins transmitting messages to the System Argos satellite network every 60 seconds for about 10 days.

· Download the latest programming software from Wildlife Computers for the tag

· Plug the custom USB cable, with the fish overmolding, into the programming port on the tag, start the program, wake-up the tag with the magnet, log-on with password Mk10
· Sync the tag’s time to UTC time using the NIST time server

· Program the tag to pre-release transmit everyday, with a daily alotment of 1440 transmissions

· Turn off histogram collection

· Exit program and select Stand-by mode

