Below is the sort of code I use. In literal terms it does not meet
your criteria. But if we twist your criteria to mean 'continue
instructions outside the interrupt' it does.

WDTCTL = WDT_ADLY_1000; // WDT 1000ms, ACLK, interval timer

while(1)
{
_BIS_SR(CPUOFF);
if(status.onesec)//to hell with interrupt protection for this test
{
status.onesec=0;
//continue processing
}

}

//watchdog Timer interrupt service routine
__interrupt void ISR_WDT(void);
WDT_ISR(ISR_WDT)
__interrupt void ISR_WDT(void)
{
status.onesec=1;
__bic_SR_register_on_exit(CPUOFF);
}