Operations Plan for 2007 Axial Seamount Cruise

Shipping/Mobilization

The AUV and its associated gear will be shipped via a 20 foot MBARI owned shipping van from Moss Landing to Astoria. Van will depart Moss Landing on July 30 AM and arrive in Astoria on July 31 AM. The van will be offloaded in Astoria using port facilities and located near where the Atlantis will tie up.

AUV Launch and Recovery crane will be transported from Seattle to Astoria. Crane will depart Seattle/SSI dock on TBD and arrive in Astoria TBD. 

Tracking

MBARI will install a Sonardyne demona USBL onto the R/V Atlantis dockside in Astoria. This will entail mounting a USBL head onto the Atlantis’ transducer pole, and cabling the head to a rack of electronics. The USBL topside will require serial interfaces to the ship’s GPS, gyro, and attitude sensors (get this info from Dave).

Launch & Recovery

Points of Contact

	Name
	Agency/Organization
	Email
	Phone

	Dave Fisichella
	WHOI/SSSG
	dfisichella@whoi.edu
	508-289-3777

	Will Sellers
	WHOI/Jason (ROV Lead on cruise)
	wsellers@whoi.edu
	508-289-2617

	Lou Marconeri
	R/V Atlantis agent in Astoria
	lmarconeri@knutsenins.com
	503-325-3721

	Daniel
	Nautronix (Atlantis LUSBL System)
	
	713-880-2848

	Bob Brown
	WHOI/ALVIN Group
	
	508-289-2786


