SPROUL – AUV Cruise Meeting
Draft Minutes
drthom@mbari.org


Overview

Priorities of Thin Layers Cruise (Aug 25 thru 1 Sept)

1. AUV operations

2. Drifters launch and recovery  (2 drifters)

3. CTD Rosette operation

Plan to do a CTD cast near the start of AUV operations, preferably at the northmost waypoint of the triangle.  Northmost waypoint preferred for weather shelter.

CTD Ops should provide:


1. Ground truthing



a.    NO3



b.    Chlorophyl


 2. Target Layers

a. we pickle

b. Scholin SHA

c. Chavez

Carole Sakamoto will provide bottles for ISUS truthing

Chris Scholin lab will provide (lots of) bottles

Ops will be running a Rib, to swap out the Zephyr crew and possibly some engineering folks, maybe someone from the Chris Scholin lab.  Also possible water sample transfer (small container size preferable).

CTD AUV 


Plan to get Iridium functional


Mod control software to do a self-restart on depth aborts


Vehicle will usually be running in bottom lock mode


Expect about 6 hours duration @ 3.5 knots per triangle


100 meters max depth

AUV will be running the Bathyphotometer and LISST


May want to adjust recovery time to around 5 AM to maximize Biolume data


Perhaps do two loops on the first round, to adjust timing

Data

Data will be “quick looks”, using ship’s email, JPEGs.  Also a possible 802.11 radio link using Cisco Airnet bridge.

Schedule

18 August
LOCO triangle AUV ops on Zephyr

19 August
Mobe’ in San Diego  

2 MBARIans:  TBD

Take Charger Supplies and Cabling

Everything else possible to minimize mobe’ time at Moss Landing

22 August
Sproul leaves San Diego for Moss Landing



48 hour run at 8 knots



Expect some weather related delay

24 August
Complete the mobe’ at Moss Landing



Plan to leave dock around 4 PM



Launch AUV by 6 PM at northmost waypoint



Recovery around Noon on 25 Aug (first run)

1 September
Return in afternoon, de-mobe’



Make sure Scripps folks have enough time to de-mobe’ in San Diego

Do we need to have an MBARIan in San Diego, or can Richard Zimmerman do the de-mobe’

Action Items

Plan to look into possible use of UNOLS SWAP system.

Need to locate sea water tap, make sure enough hose is available, for AUV battery cooling during high-current charging

Bring along a stack of CD-Rs and footballs for Data Transfer

Bring along Bean Bag Chairs

Buy a spare capture line

Build up a spare capture pole and head

Bring along a liquid nitrogen dewar

Request underway fluorometer on the Sproul  (Doug Conlin possibly has one we can use)

Find out of Richard Zimmerman needs MBARIans to assist in San Diego de-mobe’ on 3 September

