U.S. VHF CHANNELS
 

	Channel Number
	Ship Transmit MHz
	Ship Receive MHz
	Use

	01A
	156.050
	156.050
	Port Operations and Commercial, VTS. Available only in New Orleans / Lower Mississippi area.

	05A
	156.250
	156.250
	Port Operations or VTS in the Houston, New Orleans and Seattle areas.

	06
	156.300
	156.300
	Intership Safety

	07A
	156.350
	156.350
	Commercial

	08
	156.400
	156.400
	Commercial (Intership only)

	09
	156.450
	156.450
	Boater Calling. Commercial and Non-Commercial.

	10
	156.500
	156.500
	Commercial

	11
	156.550
	156.550
	Commercial. VTS in selected areas.

	12
	156.600
	156.600
	Port Operations. VTS in selected areas.

	13
	156.650
	156.650
	Intership Navigation Safety (Bridge-to-bridge). Ships >20m length maintain a listening watch on this channel in US waters.

	14
	156.700
	156.700
	Port Operations. VTS in selected areas.

	15
	--
	156.750
	Environmental (Receive only). Used by Class C EPIRBs.

	16
	156.800
	156.800
	International Distress, Safety and Calling. Ships required to carry radio, USCG, and most coast stations maintain a listening watch on this channel.

	17
	156.850
	156.850
	State & local govt maritime control

	18A
	156.900
	156.900
	Commercial

	19A
	156.950
	156.950
	Commercial

	20
	157.000
	161.600
	Port Operations (duplex)

	20A
	157.000
	157.000
	Port Operations

	21A
	157.050
	157.050
	U.S. Coast Guard only

	22A
	157.100
	157.100
	Coast Guard Liaison and Maritime Safety Information Broadcasts. Broadcasts announced on channel 16.

	23A
	157.150
	157.150
	U.S. Coast Guard only

	24
	157.200
	161.800
	Public Correspondence (Marine Operator)

	25
	157.250
	161.850
	Public Correspondence (Marine Operator)

	26
	157.300
	161.900
	Public Correspondence (Marine Operator)

	27
	157.350
	161.950
	Public Correspondence (Marine Operator)

	28
	157.400
	162.000
	Public Correspondence (Marine Operator)

	63A
	156.175
	156.175
	Port Operations and Commercial, VTS. Available only in New Orleans / Lower Mississippi area.

	65A
	156.275
	156.275
	Port Operations

	66A
	156.325
	156.325
	Port Operations

	67
	156.375
	156.375
	Commercial. Used for Bridge-to-bridge communications in lower Mississippi River. Intership only.

	68
	156.425
	156.425
	Non-Commercial

	69
	156.475
	156.475
	Non-Commercial

	70
	156.525
	156.525
	Digital Selective Calling (voice communications not allowed)

	71
	156.575
	156.575
	Non-Commercial

	72
	156.625
	156.625
	Non-Commercial (Intership only)

	73
	156.675
	156.675
	Port Operations

	74
	156.725
	156.725
	Port Operations

	77
	156.875
	156.875
	Port Operations (Intership only)

	78A
	156.925
	156.925
	Non-Commercial

	79A
	156.975
	156.975
	Commercial. Non-Commercial in Great Lakes only

	80A
	157.025
	157.025
	Commercial. Non-Commercial in Great Lakes only

	81A
	157.075
	157.075
	U.S. Government only - Environmental protection operations.

	82A
	157.125
	157.125
	U.S. Government only

	83A
	157.175
	157.175
	U.S. Coast Guard only

	84
	157.225
	161.825
	Public Correspondence (Marine Operator)

	85
	157.275
	161.875
	Public Correspondence (Marine Operator)

	86
	157.325
	161.925
	Public Correspondence (Marine Operator)

	87
	157.375
	157.375
	Public Correspondence (Marine Operator)

	88A
	157.425
	157.425
	Commercial, Intership only.

	AIS 1
	161.975
	161.975
	Automatic Identification System (AIS)


