48.00

36.00

36.00

48.00

96.00

48.00

1

1 1

1

6

8 3

3 2

2 3 7

J8

J4

J5

Spa re

J44M

J33M

J33F

Spa re

ITEM NO. QTY. PART NO. VENDOR DESCRIPTION PO ITEM NO.

1 4 MINK10Pe ne tra tor R/A-TI Se a c onn/Bra ntne r MINK10/L PNA, 6AL-4V Ti, w/ R/A Mold, 18in Te flon Hookups, Epoxy Fille d 5

2 2 EN204011 Cortla nd C/F 1x14GA STP/5x22GA STP w/ PU Ja c ke t, 36in long N/A

3 3 EN204011 Cortla nd C/F 1x14GA STP/5x22GA STP w/ PU Ja c ke t, 48in long N/A

4 2 MINK10CCP/L-SSTLS Se a c onn/Bra ntne r MINK-10-CCP/L, 316SS w/ Inline Mold 2

5 2 EN204011 Cortla nd C/F 1x14GA STP/5x22GA STP w/ PU Ja c ke t, 50ft long N/A

6 1 MINK10CCPL-TI Se a c onn/Bra ntne r MINK10-CCP/L, 6AL-4V Ti w/ Inline Mold 1

7 1 EN204011 Cortla nd C/F 1x14GA STP/5x22GA STP w/PU Ja c ke t, 96in long N/A

8 1 MINK10-CCR/L-Ti Se a c onn/Bra ntne r MINK10-CCR/L, 6AL-4V TI w/ In-Line Mold 3

600.00 4 5

600.00 4 5

D

C

B

A A

B

C

D

Monterey Bay Aquarium Research Institute

SCALE

SIZE

CAD FILE:

DWG. NO. B SHEET 1 OF 1

REV.

multibea m_sea conn_wet_ca bling

DATE

APPROVALS

DRAWN

CHECKED

ENGINEER

UNLESS OTHERWISE SPECIFIED

TOLERANCES ARE:

DO NOT SCALE DRAWING

Applica tion

NEXT ASSY

Description

BILL OF MATERIALS

1 2 3 4 5 6 7 8

8 7 6 5 4 3 2 1

THE INFORMATION CONTAINED IN THIS DRAWING IS THE SOLE PROPERTY OF MBARI ANY

REPRODUCTION IN PART OR WHOLE WITHOUT THE WRITTEN PERMISSION OF MBARI IS PROHIBITED.

REVISIONS

REV. DESCRIPTION DATE APPROVED

1 PLACE DIM

1/16

2 PLACE DIM .02 3 PLACE DIM

.005

ANGLES 1 1. DIMENSIONS ARE IN INCHES

2. DIMENSION LIMITS HELD AFTER PLATING.

3. REMOVE BURRS AND SHARP EDGES .015 MAX.

4. MACHINED FILLET RADII .0150-.030.

5. MACHINED DIAMETERS ON A COMMON

CENTERLINE CONCENTRIC WITHIN .OO5

6. PERPENDICULARITY & PARALLELISM OF

MACHINED SURFACES .002 PER INCH.

MAX .012 INCHES FOR SINGLE SURFACE.

PROJECT NO.

PROJECT

MBARI

7700 Sandholdt RD.

Moss Landing, CA 95039

PH: (831) 775-1700

Thoma s

Sibena c 5/14/03

200107

Sea floor Ma pping

1:10 MECH ENG ON TORNADO

INITIAL RELEASE

WEIGHT

5/14/03

1001970

Shop / Q.C.

Engineer

Inspector

Shop Forema n

NEXT ASSY

Number

Terminate C/F Cable to MINK10/L As Follows:

Pin # Conductor

1 14GA STP/Red

2 22GA Green&White STP/White

3 22GA Green&White STP/Green

4 22GA Blue&White STP/White

5 22GA Blue&White STP/Blue

6 22GA Orange&Green STP/Orange

7 22GA Orange&Green STP/Green

8 22GA Orange&Blue STP/Orange

9 Drain wire soldered to 14GA Shield

10 14GA STP/Green