5/6/2019 AUV Group Meeting
Upcoming Dives
May 7/May 8 – overnight CTD mission
May 9 – May 14 – Mapping at Morro Bay Windfarm
May 21/22 – I2MAP
June 3/4 – I2MAP at MARS
TRN Testing Last week
· multiple passes over Ledge with TRN inputs to Nav disabled and enabled
· need to push for long/extended test, maybe overnight at portugese ledge
· testing largely successful
· Two more testing days (6/13 and 6/28)
T50 Multibeam Testing
· Data collection at 50 meters using 60us pulse/CW mode
· 142 degree swath achieved
· No 6046
· Check to see if there are other T50 specific features to test
I2MAP testing
· MVC noise reduced
· Improved filters on power board and between penetrator and power board
· Flight control behavior at 2 knots with new trim was good
· Sea trial of new omnidirectional avtrak 2 beacon
· Tested  4K video
· Will require opening of camera to change back
· Calibrate compass
CTD mission
· Launch on May 7
· Standard run
Vehicle Status
· Start charging up all batteries today (mapper 2 in B137, mapper 1 & CTD in Bay 4)
· I2MAP
· Ethernet connection still a problem (talk to simrad about this
· Noise from lights when they are off - wierd
· Mapper 2
· Make up spare  cable between edgetech & battery (mcil8f to mcil8m)
· Make up spare cable between reson and battery (lpdil13M to mcil13f)
· Mapper 1
· adjust configuration files from TRN testing to normal runs
· test SVP logging (both vehicles)
· add higher rate speed of sound updates
· CTD
· Change tail over
· Compensator added to gulpers
· Need to trim around new configuration (adjust tail lead for  new beacon and comp)
· I2MAP
· Troubleshoot light related noise
· Improve mechanical arrangement for cable routing
· [bookmark: _GoBack]Change camera back to standard configuration
