6/14/2019 AUV Group Meeting
Recent Dives
June 6/7 – I2MAP overnite run 
June 11 thru June 17 – Crawford at sea with Doc Ricketts
June 13 – TRN Testing
Upcoming Dives
Week of June 24 or July 1 – CTD towout during this week
June 25-28 – Ocean Imaging on Western Flyer (INS, Multibeam, possibly Edgetech SBP)
July 8/9 – I2MAP overnite
July 15 – TRN
Week of July 15 – CTD towout
July 31/August  1 – I2MAP run
Possible I2MAP makeup dives in November, stay turned
Sonar Issues 
Both AUV3 sonars are back.  S/N 347 (which I’d like to use on the OI sled) initially tested out OK and passed 24 hour burn in. Glitches observed during long pulse FM operations, most likely due to brown-out of DC/DC converter. I replaced the existing  200W converter with a 350W unit. Sonar powered up OK and pinged, but output shutdown during 20ms pulse FM operations. Still troubleshooting, I think it’s the power amplifier board.
Reson RX head fixed and returning from Denmark. Scheduled delivery 6/17 (Monday)
Vehicle Status
· I2MAP
· Data from last run still being analyzed
· Dropweight deployed at some point during last week’s operation. Probably operator error. Considering changing dropweight timeout and behavior to reduce likelihood of this.
· Mapper 2
· Make up spare  cable between edgetech & battery (mcil8f to mcil8m) (ordered)
· Make up spare cable between reson and battery (lpdil13M to mcil13f) (ordered)
· Move pressure sensor, change pressure sensor to 4000m unit (Crawford)
· Mounts are done
· Need to modify T50 RX head bracket to provide clearance for pressure sensor
· Make following changes to INS/DVL software & settings (both Mapper1 & Mapper2) (Thomas) (done)
· Change maximum range of DVL to 200m
· Lower error threshold for acceptable DVL fix to .2 m/s (currently it is set very large)
· Add Kearfott control behavior to allow mission to enable/disable DVL aiding, this will allow us to keep DVL aiding disabled until vehicle reaches bottom where DVL velocities are more stable
· Improve logging of INS test messages
· Mapper 1
· Bring INS up to latest firmware revision
· Move pressure sensor, change pressure sensor to 4000m unit
· CTD vehicle
· Wire in avtrak beacon to mvc sphere for comms and power
· Troubleshoot LOPC power/comms failures
· All Tails
· Change out iridium beacons for SBD warriors
Other projects
· Boom crutch (emery) – status? – drawings hopefully out by June 19
· INS isolation board (duane)
· All functions test OK, lots of blue wires
· Corrected layout done (out to fab?)
· Provide details to duane for internal harnesses
· Picking up vehicle with other crane (Crawford)
· Spare rigging kit with us on the Carson
· Grey container paint touchup (Crawford)
· Container needs welding near corner due to forklift damage (flores/Crawford)
· Ocean imaging test sled buildup (Crawford & Schnitger)
· Get sealing screw for FO penetration out for fab (or port hole for something standard, like 7/16-20 or ½-20) (JF is fab’ing on Monday)
· Mount lidar (we should also fire up LIDAR to test)
· Fix auv3 sonars
· [bookmark: _GoBack]Open House Presentation
· Emery will be giving a talk at open house
· MBARI logo for bottom of tank (emery) (done)
