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             “A Company with Depth”

Quote Number: 7951-0

            








Date: May 4, 2006



Sales Quote for:
Delivery Point/End User:

MBARI
Please confirm details with order.

7700 Sandholdt Rd, PO Box 628


Moss Landing, CA 95039-0628


USA
Lead Time: 3 Weeks  


Contact Brian Dallas with schedule concerns.

Contact: Mr Hans Thomas


Phone: (831)775-1976
 

Fax: 

	Sales Person
	Shipping-Incoterms 2000
	Payment Terms

	Brian Dallas
	FOB-Origin
	Net 30 days, 1.5% monthly finance charge

	Description
	Quantity
	Unit Price
	Extended Price

	Acoustic Baffle for 

Teledyne Benthos Modem Interrogator, AT-408
	1
	$1,830.00
	$1,830.00


Technical Specifications

DEPTH RATING:
750 METERS

FINISH:
STANDARD MARINE PAINT 

COLOR:
ORANGE 

FLOTEC ASSEMBLY DRAWING #:
DWG-04477 REV. A  

FLOTATION MATERIAL:
Flotec-750™ Syntactic Foam  

BUOYANCY:
30 lbs. (13.6 Kg) ± 2 lbs. (0.9 Kg)

WEIGHT:
26 lbs. (11.8 Kg) Nominal
CLAMP:


                                    Ultra High Molecular Weight (UHMW) Polyethylene

BOLT ASSEMBLIES:



Titanium

This quotation is valid for your acceptance 30 Days from the above date of issue.







To accept this quotation, please fax to (207) 284-8098 with your purchase order.

Acceptance of Quote & Technical Specifications: 

________________________________________
__________
               _______

_____________________


Signature of “Authorized Agent”

Date:

 
Quantity            
Purchase Order # ________________________________________
               _______________

Print Name





Title
Flotation Technologies Terms & Conditions Apply- see attached
CORPORATE HEADQUARTERS

432 Elm Street, Biddeford, ME 04005 USA

Tel: US: 800.639.7806
Tel Int’l: +1 207.282.7749

Fax: 207.284.8098
Email: sales@flotec.com
SAL-F-002, REV-


