Phone call with Brad Speer August 30, 2013 0830
Hydrogen/Oxygen Fuel Cell power source
6mw-hr for $2.6M
High Efficiency power transfer architecture
Field rings around diameter of AUV
High Q transfer
Overpopulate Coils in dock, and have charging system control which coils are active
SSC/Dombrowski does not have a conflict
Risk Reduction Risk reduction risk reduction
PDR package
PDR Q2/2015 (April/May)
Phase 1 MBARI Role
Provide engineering support (telecom/meetings/attend PDR/quarterly design reviews)
No vehicle operations, just technical consultation in Phase 1
Phase 1 Risk reduction efforts engineering/demonstration will happen on SIO 21’’ vehicle
MBARI test tank might get used in Phase 1
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