# Static Call Graph for image .\Flash\usb_host_msc.axf

#<CALLGRAPH># ARM Linker, 4.1 [Build 644]: Last Updated: Wed Feb 22 13:59:43 2012

### Maximum Stack Usage = 312 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

_printf_f ⇒ _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- NMI_Handler ⇒ NMI_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler
- SVC_Handler ⇒ SVC_Handler
- DebugMon_Handler ⇒ DebugMon_Handler
- PendSV_Handler ⇒ PendSV_Handler
- SysTick_Handler ⇒ SysTick_Handler
- ADC_IRQHandler ⇒ ADC_IRQHandler

  ### Function Pointers

  - ADC_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - BOD_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - BusFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - CANActivity_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - CAN_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - DMA_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - DebugMon_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - EINT3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - ENET_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - HardFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2C2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - I2S_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - MCPWM_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - MemManage_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - NMI_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PLL0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PLL1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PWM1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - PendSV_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - QEI_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - RIT_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - RTC_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - Reset_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SPI_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SSP0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SSP1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SVC_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SysTick_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - SystemInit from system_lpc17xx.o(.text) referenced from startup_lpc17xx.o(.text)
  - TIMER0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - TIMER3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART0_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART1_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART2_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UART3_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - USBActivity_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - USB_IRQHandler from usbhost_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - UsageFault_Handler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - WDT_IRQHandler from startup_lpc17xx.o(.text) referenced from startup_lpc17xx.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_lpc17xx.o(.text)
  - _get_lc_ctype from lc_ctype_c.o(locale$$code) referenced from rt_ctype_table.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - _sputc from _sputc.o(.text) referenced from c89vsprintf.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __rt_entry
  - >> __scatterload

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_n (Thumb, 0 bytes, Stack size unknown bytes, _printf_n.o(.ARM.Collect$$_printf_percent$$00000001))
  [Calls]

  - >> _printf_charcount

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_p (Thumb, 0 bytes, Stack size unknown bytes, _printf_p.o(.ARM.Collect$$_printf_percent$$00000002))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _printf_p ⇒ _printf_hex_ptr ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_hex_ptr

  _printf_f (Thumb, 0 bytes, Stack size unknown bytes, _printf_f.o(.ARM.Collect$$_printf_percent$$00000003))
  [Stack]

  - Max Depth = 312 + Unknown Stack Size
  - Call Chain = _printf_f ⇒ _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec

  _printf_e (Thumb, 0 bytes, Stack size unknown bytes, _printf_e.o(.ARM.Collect$$_printf_percent$$00000004))
  [Stack]

  - Max Depth = 312 + Unknown Stack Size
  - Call Chain = _printf_e ⇒ _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec

  _printf_g (Thumb, 0 bytes, Stack size unknown bytes, _printf_g.o(.ARM.Collect$$_printf_percent$$00000005))
  [Stack]

  - Max Depth = 312 + Unknown Stack Size
  - Call Chain = _printf_g ⇒ _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec

  _printf_a (Thumb, 0 bytes, Stack size unknown bytes, _printf_a.o(.ARM.Collect$$_printf_percent$$00000006))

  _printf_ll (Thumb, 0 bytes, Stack size unknown bytes, _printf_ll.o(.ARM.Collect$$_printf_percent$$00000007))

  _printf_i (Thumb, 0 bytes, Stack size unknown bytes, _printf_i.o(.ARM.Collect$$_printf_percent$$00000008))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_i ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_d (Thumb, 0 bytes, Stack size unknown bytes, _printf_d.o(.ARM.Collect$$_printf_percent$$00000009))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_d ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_u (Thumb, 0 bytes, Stack size unknown bytes, _printf_u.o(.ARM.Collect$$_printf_percent$$0000000A))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_u ⇒ _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_dec

  _printf_o (Thumb, 0 bytes, Stack size unknown bytes, _printf_o.o(.ARM.Collect$$_printf_percent$$0000000B))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _printf_o ⇒ _printf_int_oct ⇒ _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_oct

  _printf_x (Thumb, 0 bytes, Stack size unknown bytes, _printf_x.o(.ARM.Collect$$_printf_percent$$0000000C))
  [Stack]

  - Max Depth = 80 + Unknown Stack Size
  - Call Chain = _printf_x ⇒ _printf_int_hex ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_hex

  _printf_lli (Thumb, 0 bytes, Stack size unknown bytes, _printf_lli.o(.ARM.Collect$$_printf_percent$$0000000D))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_lli ⇒ _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_dec

  _printf_lld (Thumb, 0 bytes, Stack size unknown bytes, _printf_lld.o(.ARM.Collect$$_printf_percent$$0000000E))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_lld ⇒ _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_dec

  _printf_llu (Thumb, 0 bytes, Stack size unknown bytes, _printf_llu.o(.ARM.Collect$$_printf_percent$$0000000F))
  [Stack]

  - Max Depth = 72 + Unknown Stack Size
  - Call Chain = _printf_llu ⇒ _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_dec

  _printf_llo (Thumb, 0 bytes, Stack size unknown bytes, _printf_llo.o(.ARM.Collect$$_printf_percent$$00000010))
  [Stack]

  - Max Depth = 56 + Unknown Stack Size
  - Call Chain = _printf_llo ⇒ _printf_ll_oct ⇒ _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_ll_oct

  _printf_llx (Thumb, 0 bytes, Stack size unknown bytes, _printf_llx.o(.ARM.Collect$$_printf_percent$$00000011))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _printf_llx ⇒ _printf_ll_hex ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_ll_hex

  _printf_l (Thumb, 0 bytes, Stack size unknown bytes, _printf_l.o(.ARM.Collect$$_printf_percent$$00000012))

  _printf_c (Thumb, 0 bytes, Stack size unknown bytes, _printf_c.o(.ARM.Collect$$_printf_percent$$00000013))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = _printf_c ⇒ _printf_char ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_char

  _printf_s (Thumb, 0 bytes, Stack size unknown bytes, _printf_s.o(.ARM.Collect$$_printf_percent$$00000014))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = _printf_s ⇒ _printf_string ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_string

  _printf_lc (Thumb, 0 bytes, Stack size unknown bytes, _printf_lc.o(.ARM.Collect$$_printf_percent$$00000015))
  [Stack]

  - Max Depth = 88 + Unknown Stack Size
  - Call Chain = _printf_lc ⇒ _printf_wchar ⇒ _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_wchar

  _printf_ls (Thumb, 0 bytes, Stack size unknown bytes, _printf_ls.o(.ARM.Collect$$_printf_percent$$00000016))
  [Stack]

  - Max Depth = 88 + Unknown Stack Size
  - Call Chain = _printf_ls ⇒ _printf_wstring ⇒ _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_wstring

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_lib_init ⇒ _fp_init
  [Calls]
  - >> _fp_init
  [Called By]
  - >> __rt_entry_li

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000006))

  __rt_lib_init_lc_common (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000B))
  [Calls]

  - >> __rt_locale

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000008))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000D))

  __rt_lib_init_lc_ctype_2 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_lib_init_lc_ctype_2 ⇒ _get_lc_ctype
  [Calls]
  - >> _get_lc_ctype

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000F))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_numeric_2 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000012))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_lib_init_lc_numeric_2 ⇒ _get_lc_numeric
  [Calls]
  - >> _get_lc_numeric

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002A))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000028))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002F))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __main
  - >> __scatterload_rt2

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_li ⇒ __rt_lib_init ⇒ _fp_init
  [Calls]
  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 268 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ Main_Copy ⇒ FILE_Write ⇒ FAT_ClusWrite ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> exit
  - >> main

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> SVC_Handler
  [Called By]
  - >> SVC_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> DebugMon_Handler
  [Called By]
  - >> DebugMon_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> SysTick_Handler
  [Called By]
  - >> SysTick_Handler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  BOD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CANActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  CAN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  DMA_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  EINT3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  ENET_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2C2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  I2S_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  MCPWM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PLL0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PLL1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  PWM1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  QEI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  RIT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SSP0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  SSP1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  TIMER3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  UART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  USBActivity_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  WDT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_lpc17xx.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __c89vsprintf (Thumb, 32 bytes, Stack size 16 bytes, c89vsprintf.o(.text))
  [Stack]

  - Max Depth = 120 + Unknown Stack Size
  - Call Chain = __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _sputc
  - >> _printf_char_common
  [Called By]
  - >> UART_Printf

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  _printf_pre_padding (Thumb, 44 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_pre_padding
  [Called By]
  - >> _printf_fp_infnan
  - >> _printf_fp_dec_real
  - >> _printf_int_common
  - >> _printf_wctomb
  - >> _printf_str

  _printf_post_padding (Thumb, 36 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_post_padding
  [Called By]
  - >> _printf_fp_infnan
  - >> _printf_fp_dec_real
  - >> _printf_int_common
  - >> _printf_wctomb
  - >> _printf_str

  _printf_truncate_signed (Thumb, 18 bytes, Stack size 0 bytes, _printf_truncate.o(.text))
  [Called By]

  - >> _printf_int_dec

  _printf_truncate_unsigned (Thumb, 18 bytes, Stack size 0 bytes, _printf_truncate.o(.text))
  [Called By]

  - >> _printf_int_hex
  - >> _printf_int_oct
  - >> _printf_int_dec

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, _sputc.o(.text))
  [Called By]

  - >> __c89vsprintf
  [Address Reference Count : 1]
  - c89vsprintf.o(.text)

  SystemCoreClockUpdate (Thumb, 316 bytes, Stack size 0 bytes, system_lpc17xx.o(.text))
  [Called By]

  - >> main

  SystemInit (Thumb, 296 bytes, Stack size 0 bytes, system_lpc17xx.o(.text))
  [Address Reference Count : 1]

  - startup_lpc17xx.o(.text)

  FAT_GetFATType (Thumb, 52 bytes, Stack size 0 bytes, usbhost_fat.o(.text))
  [Called By]

  - >> FAT_Init

  FAT_Init (Thumb, 360 bytes, Stack size 24 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = FAT_Init ⇒ UART_Printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> UART_Printf
  - >> ReadLE32U
  - >> ReadLE16U
  - >> MS_BulkRecv
  - >> FAT_GetFATType
  [Called By]
  - >> main

  FAT_PutSFN (Thumb, 230 bytes, Stack size 16 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = FAT_PutSFN ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> MS_BulkSend
  - >> MS_BulkRecv
  [Called By]
  - >> FAT_CreateEntry

  FAT_ChkEntType (Thumb, 34 bytes, Stack size 0 bytes, usbhost_fat.o(.text))
  [Called By]

  - >> FAT_FindEntry
  - >> FAT_GetFreeEntry

  FAT_GetFreeEntry (Thumb, 122 bytes, Stack size 24 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = FAT_GetFreeEntry ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> MS_BulkRecv
  - >> FAT_ChkEntType
  [Called By]
  - >> FAT_CreateEntry

  FAT_StrCaseCmp (Thumb, 80 bytes, Stack size 0 bytes, usbhost_fat.o(.text))
  [Called By]

  - >> FAT_FindEntry

  FAT_GetSfnExt (Thumb, 92 bytes, Stack size 0 bytes, usbhost_fat.o(.text))
  [Called By]

  - >> FAT_GetSFN

  FAT_GetSfnName (Thumb, 122 bytes, Stack size 0 bytes, usbhost_fat.o(.text))
  [Called By]

  - >> FAT_GetSFN

  FAT_GetSFN (Thumb, 82 bytes, Stack size 20 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = FAT_GetSFN
  [Calls]
  - >> FAT_GetSfnName
  - >> FAT_GetSfnExt
  [Called By]
  - >> FAT_FindEntry

  FAT_FindEntry (Thumb, 164 bytes, Stack size 40 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 132
  - Call Chain = FAT_FindEntry ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> ReadLE32U
  - >> ReadLE16U
  - >> MS_BulkRecv
  - >> FAT_GetSFN
  - >> FAT_StrCaseCmp
  - >> FAT_ChkEntType
  [Called By]
  - >> FILE_Open
  - >> FAT_CreateEntry

  FAT_CreateEntry (Thumb, 48 bytes, Stack size 16 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 148
  - Call Chain = FAT_CreateEntry ⇒ FAT_FindEntry ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> FAT_FindEntry
  - >> FAT_GetFreeEntry
  - >> FAT_PutSFN
  [Called By]
  - >> FILE_Open

  FILE_Open (Thumb, 122 bytes, Stack size 24 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 172
  - Call Chain = FILE_Open ⇒ FAT_CreateEntry ⇒ FAT_FindEntry ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> FAT_CreateEntry
  - >> FAT_FindEntry
  [Called By]
  - >> Main_Write
  - >> Main_Read
  - >> Main_Copy

  FAT_ClusRead (Thumb, 312 bytes, Stack size 64 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 156
  - Call Chain = FAT_ClusRead ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> MS_BulkRecv
  [Called By]
  - >> FILE_Read

  FAT_GetNextClus (Thumb, 98 bytes, Stack size 24 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = FAT_GetNextClus ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> ReadLE16U
  - >> MS_BulkRecv
  [Called By]
  - >> FAT_GetEndClus
  - >> FILE_Read

  FILE_Read (Thumb, 270 bytes, Stack size 40 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 196
  - Call Chain = FILE_Read ⇒ FAT_ClusRead ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> FAT_GetNextClus
  - >> FAT_ClusRead
  [Called By]
  - >> Main_Write
  - >> Main_Read
  - >> Main_Copy

  FAT_UpdateFAT (Thumb, 90 bytes, Stack size 24 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = FAT_UpdateFAT ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> WriteLE16U
  - >> MS_BulkSend
  - >> MS_BulkRecv
  [Called By]
  - >> FILE_Write

  FAT_GetFreeClus (Thumb, 112 bytes, Stack size 24 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 116
  - Call Chain = FAT_GetFreeClus ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> ReadLE16U
  - >> MS_BulkRecv
  [Called By]
  - >> FILE_Write

  FAT_ClusWrite (Thumb, 336 bytes, Stack size 64 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 156
  - Call Chain = FAT_ClusWrite ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> MS_BulkSend
  - >> MS_BulkRecv
  [Called By]
  - >> FILE_Write

  FAT_GetEndClus (Thumb, 28 bytes, Stack size 16 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 132
  - Call Chain = FAT_GetEndClus ⇒ FAT_GetNextClus ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> FAT_GetNextClus
  [Called By]
  - >> FILE_Write

  FILE_Write (Thumb, 290 bytes, Stack size 40 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 196
  - Call Chain = FILE_Write ⇒ FAT_ClusWrite ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> WriteLE16U
  - >> MS_BulkSend
  - >> MS_BulkRecv
  - >> FAT_GetEndClus
  - >> FAT_ClusWrite
  - >> FAT_GetFreeClus
  - >> FAT_UpdateFAT
  [Called By]
  - >> Main_Write
  - >> Main_Copy

  FAT_UpdateEntry (Thumb, 60 bytes, Stack size 16 bytes, usbhost_fat.o(.text), UNUSED)
  [Calls]

  - >> WriteLE32U
  - >> MS_BulkSend
  - >> MS_BulkRecv

  FILE_Close (Thumb, 100 bytes, Stack size 16 bytes, usbhost_fat.o(.text))
  [Stack]

  - Max Depth = 108
  - Call Chain = FILE_Close ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> WriteLE32U
  - >> MS_BulkSend
  - >> MS_BulkRecv
  [Called By]
  - >> Main_Write
  - >> Main_Read
  - >> Main_Copy

  Host_DelayUS (Thumb, 22 bytes, Stack size 0 bytes, usbhost_lpc17xx.o(.text))
  [Called By]

  - >> Host_DelayMS

  Host_DelayMS (Thumb, 32 bytes, Stack size 8 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = Host_DelayMS
  [Calls]
  - >> Host_DelayUS
  [Called By]
  - >> Host_EnumDev
  - >> Host_Init

  Host_HCCAInit (Thumb, 36 bytes, Stack size 0 bytes, usbhost_lpc17xx.o(.text))
  [Called By]

  - >> Host_Init

  Host_TDInit (Thumb, 14 bytes, Stack size 0 bytes, usbhost_lpc17xx.o(.text))
  [Called By]

  - >> Host_Init

  Host_EDInit (Thumb, 14 bytes, Stack size 0 bytes, usbhost_lpc17xx.o(.text))
  [Called By]

  - >> Host_Init

  Host_Init (Thumb, 372 bytes, Stack size 16 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = Host_Init ⇒ UART_Printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> Host_EDInit
  - >> Host_TDInit
  - >> Host_HCCAInit
  - >> Host_DelayMS
  - >> UART_Printf
  [Called By]
  - >> main

  USB_IRQHandler (Thumb, 412 bytes, Stack size 16 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = USB_IRQHandler ⇒ UART_Printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> UART_Printf
  [Address Reference Count : 1]
  - startup_lpc17xx.o(RESET)

  Host_WDHWait (Thumb, 20 bytes, Stack size 0 bytes, usbhost_lpc17xx.o(.text))
  [Called By]

  - >> Host_ProcessTD

  Host_ProcessTD (Thumb, 468 bytes, Stack size 16 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = Host_ProcessTD
  [Calls]
  - >> Host_WDHWait
  [Called By]
  - >> MS_TestUnitReady
  - >> MS_GetSenseInfo
  - >> MS_ReadCapacity
  - >> MS_Inquire
  - >> Host_CtrlRecv
  - >> Host_CtrlSend
  - >> MS_BulkSend
  - >> MS_BulkRecv

  WriteLE16U (Thumb, 16 bytes, Stack size 12 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = WriteLE16U
  [Called By]
  - >> Host_FillSetup
  - >> FILE_Write
  - >> FAT_UpdateFAT

  Host_FillSetup (Thumb, 96 bytes, Stack size 28 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = Host_FillSetup ⇒ WriteLE16U
  [Calls]
  - >> WriteLE16U
  [Called By]
  - >> Host_CtrlRecv
  - >> Host_CtrlSend

  Host_CtrlSend (Thumb, 98 bytes, Stack size 36 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = Host_CtrlSend ⇒ Host_FillSetup ⇒ WriteLE16U
  [Calls]
  - >> Host_FillSetup
  - >> Host_ProcessTD
  [Called By]
  - >> Host_EnumDev

  ReadLE16U (Thumb, 22 bytes, Stack size 8 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ReadLE16U
  [Called By]
  - >> MS_ParseConfiguration
  - >> Host_EnumDev
  - >> FAT_GetFreeClus
  - >> FAT_GetNextClus
  - >> FAT_FindEntry
  - >> FAT_Init

  Host_CtrlRecv (Thumb, 98 bytes, Stack size 36 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = Host_CtrlRecv ⇒ Host_FillSetup ⇒ WriteLE16U
  [Calls]
  - >> Host_FillSetup
  - >> Host_ProcessTD
  [Called By]
  - >> MS_GetMaxLUN
  - >> Host_EnumDev

  Host_EnumDev (Thumb, 432 bytes, Stack size 24 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 184 + Unknown Stack Size
  - Call Chain = Host_EnumDev ⇒ MS_ParseConfiguration ⇒ UART_Printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> MS_ParseConfiguration
  - >> Host_CtrlRecv
  - >> Host_CtrlSend
  - >> Host_DelayMS
  - >> UART_Printf
  - >> ReadLE16U
  [Called By]
  - >> main

  ReadLE32U (Thumb, 32 bytes, Stack size 8 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ReadLE32U
  [Called By]
  - >> FAT_FindEntry
  - >> FAT_Init

  WriteLE32U (Thumb, 28 bytes, Stack size 12 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = WriteLE32U
  [Called By]
  - >> Fill_MSCommand
  - >> FILE_Close
  - >> FAT_UpdateEntry

  ReadBE32U (Thumb, 32 bytes, Stack size 8 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = ReadBE32U
  [Called By]
  - >> MS_ReadCapacity

  WriteBE32U (Thumb, 28 bytes, Stack size 12 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = WriteBE32U
  [Called By]
  - >> Fill_MSCommand

  ReadBE16U (Thumb, 22 bytes, Stack size 8 bytes, usbhost_lpc17xx.o(.text), UNUSED)

  WriteBE16U (Thumb, 16 bytes, Stack size 12 bytes, usbhost_lpc17xx.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = WriteBE16U
  [Called By]
  - >> Fill_MSCommand

  Fill_MSCommand (Thumb, 206 bytes, Stack size 40 bytes, usbhost_ms.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> WriteBE16U
  - >> WriteBE32U
  - >> WriteLE32U
  [Called By]
  - >> MS_TestUnitReady
  - >> MS_GetSenseInfo
  - >> MS_ReadCapacity
  - >> MS_Inquire
  - >> MS_BulkSend
  - >> MS_BulkRecv

  MS_Inquire (Thumb, 160 bytes, Stack size 24 bytes, usbhost_ms.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = MS_Inquire ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> Fill_MSCommand
  - >> Host_ProcessTD
  [Called By]
  - >> MS_Init

  MS_ReadCapacity (Thumb, 142 bytes, Stack size 24 bytes, usbhost_ms.o(.text))
  [Stack]

  - Max Depth = 76
  - Call Chain = MS_ReadCapacity ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> Fill_MSCommand
  - >> ReadBE32U
  - >> Host_ProcessTD
  [Called By]
  - >> MS_Init

  MS_GetSenseInfo (Thumb, 106 bytes, Stack size 16 bytes, usbhost_ms.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = MS_GetSenseInfo ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> Fill_MSCommand
  - >> Host_ProcessTD
  [Called By]
  - >> MS_Init

  MS_TestUnitReady (Thumb, 82 bytes, Stack size 16 bytes, usbhost_ms.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = MS_TestUnitReady ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> Fill_MSCommand
  - >> Host_ProcessTD
  [Called By]
  - >> MS_Init

  MS_GetMaxLUN (Thumb, 30 bytes, Stack size 16 bytes, usbhost_ms.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = MS_GetMaxLUN ⇒ Host_CtrlRecv ⇒ Host_FillSetup ⇒ WriteLE16U
  [Calls]
  - >> Host_CtrlRecv
  [Called By]
  - >> MS_Init

  MS_Init (Thumb, 100 bytes, Stack size 24 bytes, usbhost_ms.o(.text))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = MS_Init ⇒ UART_Printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> MS_GetMaxLUN
  - >> MS_TestUnitReady
  - >> MS_GetSenseInfo
  - >> MS_ReadCapacity
  - >> MS_Inquire
  - >> UART_Printf
  [Called By]
  - >> main

  MS_ParseConfiguration (Thumb, 342 bytes, Stack size 16 bytes, usbhost_ms.o(.text))
  [Stack]

  - Max Depth = 160 + Unknown Stack Size
  - Call Chain = MS_ParseConfiguration ⇒ UART_Printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> UART_Printf
  - >> ReadLE16U
  [Called By]
  - >> Host_EnumDev

  MS_BulkRecv (Thumb, 162 bytes, Stack size 40 bytes, usbhost_ms.o(.text))
  [Stack]

  - Max Depth = 92
  - Call Chain = MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> Fill_MSCommand
  - >> Host_ProcessTD
  [Called By]
  - >> FILE_Close
  - >> FAT_UpdateEntry
  - >> FILE_Write
  - >> FAT_ClusWrite
  - >> FAT_GetFreeClus
  - >> FAT_UpdateFAT
  - >> FAT_GetNextClus
  - >> FAT_ClusRead
  - >> FAT_FindEntry
  - >> FAT_GetFreeEntry
  - >> FAT_PutSFN
  - >> FAT_Init

  MS_BulkSend (Thumb, 128 bytes, Stack size 32 bytes, usbhost_ms.o(.text))
  [Stack]

  - Max Depth = 84
  - Call Chain = MS_BulkSend ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> Fill_MSCommand
  - >> Host_ProcessTD
  [Called By]
  - >> FILE_Close
  - >> FAT_UpdateEntry
  - >> FILE_Write
  - >> FAT_ClusWrite
  - >> FAT_UpdateFAT
  - >> FAT_PutSFN

  UART_Init (Thumb, 118 bytes, Stack size 12 bytes, usbhost_uart.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = UART_Init
  [Called By]
  - >> main

  UART_PrintChar (Thumb, 18 bytes, Stack size 0 bytes, usbhost_uart.o(.text))
  [Called By]

  - >> UART_PrintStr

  UART_PrintStr (Thumb, 52 bytes, Stack size 4 bytes, usbhost_uart.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = UART_PrintStr
  [Calls]
  - >> UART_PrintChar
  [Called By]
  - >> UART_Printf

  UART_Printf (Thumb, 36 bytes, Stack size 24 bytes, usbhost_uart.o(.text))
  [Stack]

  - Max Depth = 144 + Unknown Stack Size
  - Call Chain = UART_Printf ⇒ __c89vsprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> __c89vsprintf
  - >> UART_PrintStr
  [Called By]
  - >> Main_Write
  - >> Main_Read
  - >> Main_Copy
  - >> MS_Init
  - >> MS_ParseConfiguration
  - >> Host_EnumDev
  - >> USB_IRQHandler
  - >> Host_Init
  - >> FAT_Init

  Main_Copy (Thumb, 120 bytes, Stack size 16 bytes, usb_host_msc.o(.text))
  [Stack]

  - Max Depth = 212 + Unknown Stack Size
  - Call Chain = Main_Copy ⇒ FILE_Write ⇒ FAT_ClusWrite ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> UART_Printf
  - >> FILE_Close
  - >> FILE_Write
  - >> FILE_Read
  - >> FILE_Open
  [Called By]
  - >> main

  main (Thumb, 74 bytes, Stack size 56 bytes, usb_host_msc.o(.text))
  [Stack]

  - Max Depth = 268 + Unknown Stack Size
  - Call Chain = main ⇒ Main_Copy ⇒ FILE_Write ⇒ FAT_ClusWrite ⇒ MS_BulkRecv ⇒ Fill_MSCommand ⇒ WriteBE16U
  [Calls]
  - >> Main_Copy
  - >> UART_Init
  - >> MS_Init
  - >> Host_EnumDev
  - >> Host_Init
  - >> FAT_Init
  - >> SystemCoreClockUpdate
  [Called By]
  - >> __rt_entry_main

  Main_Read (Thumb, 74 bytes, Stack size 16 bytes, usb_host_msc.o(.text), UNUSED)
  [Calls]

  - >> UART_Printf
  - >> FILE_Close
  - >> FILE_Read
  - >> FILE_Open

  Main_Write (Thumb, 136 bytes, Stack size 24 bytes, usb_host_msc.o(.text), UNUSED)
  [Calls]

  - >> UART_Printf
  - >> FILE_Close
  - >> FILE_Write
  - >> FILE_Read
  - >> FILE_Open

  _printf_str (Thumb, 82 bytes, Stack size 16 bytes, _printf_str.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_cs_common

  _printf_int_dec (Thumb, 102 bytes, Stack size 24 bytes, _printf_dec.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = _printf_int_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  - >> _printf_truncate_unsigned
  - >> _printf_truncate_signed
  [Called By]
  - >> _printf_u
  - >> _printf_d
  - >> _printf_i

  _printf_charcount (Thumb, 42 bytes, Stack size 0 bytes, _printf_charcount.o(.text))
  [Called By]

  - >> _printf_n

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> __c89vsprintf

  _printf_wctomb (Thumb, 182 bytes, Stack size 56 bytes, _printf_wctomb.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _wcrtomb
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_lcs_common

  _printf_longlong_dec (Thumb, 104 bytes, Stack size 24 bytes, _printf_longlong_dec.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = _printf_longlong_dec ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  - >> _ll_udiv10
  [Called By]
  - >> _printf_llu
  - >> _printf_lld
  - >> _printf_lli

  _printf_longlong_oct (Thumb, 76 bytes, Stack size 8 bytes, _printf_oct_int_ll.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_ll_oct
  - >> _printf_int_oct

  _printf_int_oct (Thumb, 24 bytes, Stack size 8 bytes, _printf_oct_int_ll.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_int_oct ⇒ _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_oct
  - >> _printf_truncate_unsigned
  [Called By]
  - >> _printf_o

  _printf_ll_oct (Thumb, 12 bytes, Stack size 0 bytes, _printf_oct_int_ll.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = _printf_ll_oct ⇒ _printf_longlong_oct ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_oct
  [Called By]
  - >> _printf_llo

  _printf_longlong_hex (Thumb, 92 bytes, Stack size 16 bytes, _printf_hex_int_ll_ptr.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_hex_ptr
  - >> _printf_ll_hex
  - >> _printf_int_hex

  _printf_int_hex (Thumb, 28 bytes, Stack size 16 bytes, _printf_hex_int_ll_ptr.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = _printf_int_hex ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_hex
  - >> _printf_truncate_unsigned
  [Called By]
  - >> _printf_x

  _printf_ll_hex (Thumb, 12 bytes, Stack size 0 bytes, _printf_hex_int_ll_ptr.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_ll_hex ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_hex
  [Called By]
  - >> _printf_llx

  _printf_hex_ptr (Thumb, 18 bytes, Stack size 0 bytes, _printf_hex_int_ll_ptr.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_hex_ptr ⇒ _printf_longlong_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_longlong_hex
  [Called By]
  - >> _printf_p

  __printf (Thumb, 408 bytes, Stack size 40 bytes, __printf_flags_ss_wp.o(.text))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  - >> _is_digit
  [Called By]
  - >> _printf_char_common

  _ll_udiv10 (Thumb, 138 bytes, Stack size 12 bytes, lludiv10.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = _ll_udiv10
  [Called By]
  - >> _fp_digits
  - >> _printf_longlong_dec

  _printf_int_common (Thumb, 182 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_longlong_hex
  - >> _printf_longlong_oct
  - >> _printf_longlong_dec
  - >> _printf_int_dec

  __lib_sel_fp_printf (Thumb, 2 bytes, Stack size 0 bytes, _printf_fp_dec.o(.text), UNUSED)

  _printf_fp_dec_real (Thumb, 646 bytes, Stack size 104 bytes, _printf_fp_dec.o(.text))
  [Stack]

  - Max Depth = 312
  - Call Chain = _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> __ARM_fpclassify
  - >> _printf_fp_infnan
  - >> __rt_locale
  - >> _fp_digits
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_fp_dec

  _printf_cs_common (Thumb, 20 bytes, Stack size 8 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_str
  [Called By]
  - >> _printf_string
  - >> _printf_char

  _printf_char (Thumb, 16 bytes, Stack size 0 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_char ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_cs_common
  [Called By]
  - >> _printf_c

  _printf_string (Thumb, 8 bytes, Stack size 0 bytes, _printf_char.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_string ⇒ _printf_cs_common ⇒ _printf_str ⇒ _printf_post_padding
  [Calls]
  - >> _printf_cs_common
  [Called By]
  - >> _printf_s

  _printf_lcs_common (Thumb, 20 bytes, Stack size 8 bytes, _printf_wchar.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_wctomb
  [Called By]
  - >> _printf_wstring
  - >> _printf_wchar

  _printf_wchar (Thumb, 16 bytes, Stack size 0 bytes, _printf_wchar.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = _printf_wchar ⇒ _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_lcs_common
  [Called By]
  - >> _printf_lc

  _printf_wstring (Thumb, 8 bytes, Stack size 0 bytes, _printf_wchar.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = _printf_wstring ⇒ _printf_lcs_common ⇒ _printf_wctomb ⇒ _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> _printf_lcs_common
  [Called By]
  - >> _printf_ls

  _wcrtomb (Thumb, 64 bytes, Stack size 16 bytes, _wcrtomb.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = _wcrtomb ⇒ __rt_ctype_table
  [Calls]
  - >> __rt_ctype_table
  [Called By]
  - >> _printf_wctomb

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  __rt_ctype_table (Thumb, 16 bytes, Stack size 8 bytes, rt_ctype_table.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __rt_ctype_table
  [Calls]
  - >> __rt_locale
  [Called By]
  - >> _wcrtomb

  __rt_locale (Thumb, 8 bytes, Stack size 0 bytes, rt_locale_intlibspace.o(.text))
  [Called By]

  - >> __rt_ctype_table
  - >> _printf_fp_dec_real
  - >> __rt_lib_init_lc_common

  _printf_fp_infnan (Thumb, 108 bytes, Stack size 24 bytes, _printf_fp_infnan.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _printf_fp_infnan ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_fp_dec_real

  _btod_etento (Thumb, 222 bytes, Stack size 72 bytes, bigflt0.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _btod_emul
  - >> _btod_ediv
  [Called By]
  - >> _fp_digits

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  strcmp (Thumb, 128 bytes, Stack size 0 bytes, strcmpv7m.o(.text))
  [Called By]

  - >> _get_lc_ctype
  - >> _get_lc_numeric

  __rt_fp_status_addr (Thumb, 8 bytes, Stack size 0 bytes, rt_fp_status_addr_intlibspace.o(.text))
  [Called By]

  - >> _fp_init

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  _btod_d2e (Thumb, 62 bytes, Stack size 0 bytes, btod.o(CL$$btod_d2e))
  [Calls]

  - >> _d2e_norm_op1
  [Called By]
  - >> _fp_digits

  _d2e_denorm_low (Thumb, 70 bytes, Stack size 0 bytes, btod.o(CL$$btod_d2e_denorm_low))
  [Called By]

  - >> _d2e_norm_op1

  _d2e_norm_op1 (Thumb, 96 bytes, Stack size 0 bytes, btod.o(CL$$btod_d2e_norm_op1))
  [Calls]

  - >> _d2e_denorm_low
  [Called By]
  - >> _btod_d2e

  __btod_div_common (Thumb, 696 bytes, Stack size 24 bytes, btod.o(CL$$btod_div_common))
  [Stack]

  - Max Depth = 24
  - Call Chain = __btod_div_common
  [Called By]
  - >> _btod_ediv

  _e2e (Thumb, 198 bytes, Stack size 24 bytes, btod.o(CL$$btod_e2e))
  [Stack]

  - Max Depth = 24
  - Call Chain = _e2e
  [Called By]
  - >> _btod_emul
  - >> _btod_ediv

  _btod_ediv (Thumb, 40 bytes, Stack size 24 bytes, btod.o(CL$$btod_ediv))
  [Stack]

  - Max Depth = 48
  - Call Chain = _btod_ediv ⇒ _e2e
  [Calls]
  - >> _e2e
  - >> __btod_div_common
  [Called By]
  - >> _btod_etento
  - >> _fp_digits

  _btod_emul (Thumb, 40 bytes, Stack size 24 bytes, btod.o(CL$$btod_emul))
  [Stack]

  - Max Depth = 48
  - Call Chain = _btod_emul ⇒ _e2e
  [Calls]
  - >> __btod_mult_common
  - >> _e2e
  [Called By]
  - >> _btod_etento
  - >> _fp_digits

  __btod_mult_common (Thumb, 580 bytes, Stack size 16 bytes, btod.o(CL$$btod_mult_common))
  [Stack]

  - Max Depth = 16
  - Call Chain = __btod_mult_common
  [Called By]
  - >> _btod_emul

  __ARM_fpclassify (Thumb, 40 bytes, Stack size 0 bytes, fpclassify.o(i.__ARM_fpclassify))
  [Called By]

  - >> _printf_fp_dec_real

  _is_digit (Thumb, 14 bytes, Stack size 0 bytes, __printf_wp.o(i._is_digit))
  [Called By]

  - >> __printf

  _get_lc_numeric (Thumb, 44 bytes, Stack size 8 bytes, lc_numeric_c.o(locale$$code))
  [Stack]

  - Max Depth = 8
  - Call Chain = _get_lc_numeric
  [Calls]
  - >> strcmp
  [Called By]
  - >> __rt_lib_init_lc_numeric_2

  _get_lc_ctype (Thumb, 44 bytes, Stack size 8 bytes, lc_ctype_c.o(locale$$code))
  [Stack]

  - Max Depth = 8
  - Call Chain = _get_lc_ctype
  [Calls]
  - >> strcmp
  [Called By]
  - >> __rt_lib_init_lc_ctype_2
  [Address Reference Count : 1]
  - rt_ctype_table.o(.text)

  _fp_init (Thumb, 14 bytes, Stack size 8 bytes, fpinit.o(x$fpl$fpinit))
  [Stack]

  - Max Depth = 8
  - Call Chain = _fp_init
  [Calls]
  - >> __rt_fp_status_addr
  [Called By]
  - >> __rt_lib_init

  __fplib_config_pureend_doubles (Thumb, 0 bytes, Stack size unknown bytes, fpinit.o(x$fpl$fpinit), UNUSED)

  _printf_fp_dec (Thumb, 4 bytes, Stack size 0 bytes, printf1.o(x$fpl$printf1))
  [Stack]

  - Max Depth = 312
  - Call Chain = _printf_fp_dec ⇒ _printf_fp_dec_real ⇒ _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _printf_fp_dec_real
  [Called By]
  - >> _printf_g
  - >> _printf_e
  - >> _printf_f

  __I$use$fp (Thumb, 0 bytes, Stack size unknown bytes, usenofp.o(x$fpl$usenofp), UNUSED)

  ### Local Symbols

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  _fp_digits (Thumb, 418 bytes, Stack size 88 bytes, _printf_fp_dec.o(.text))
  [Stack]

  - Max Depth = 208
  - Call Chain = _fp_digits ⇒ _btod_etento ⇒ _btod_emul ⇒ _e2e
  [Calls]
  - >> _btod_emul
  - >> _btod_ediv
  - >> _btod_d2e
  - >> _btod_etento
  - >> _ll_udiv10
  [Called By]
  - >> _printf_fp_dec_real

  ### Undefined Global Symbols