- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_biquad_cascade_df1_init_q15.c

Go to the documentation of this file.

    00001 /*-----------------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        29. November 2010
    00005 * $Revision:    V1.0.3
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_biquad_cascade_df1_init_q15.c
    00009 *
    00010 * Description:  Q15 Biquad cascade DirectFormI(DF1) filter initialization function.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3
    00013 *
    00014 * Version 1.0.3 2010/11/29
    00015 *    Re-organized the CMSIS folders and updated documentation.
    00016 *
    00017 * Version 1.0.2 2010/11/11
    00018 *    Documentation updated.
    00019 *
    00020 * Version 1.0.1 2010/10/05
    00021 *    Production release and review comments incorporated.
    00022 *
    00023 * Version 1.0.0 2010/09/20
    00024 *    Production release and review comments incorporated.
    00025 *
    00026 * Version 0.0.5  2010/04/26
    00027 *    incorporated review comments and updated with latest CMSIS layer
    00028 *
    00029 * Version 0.0.3  2010/03/10
    00030 *    Initial version
    00031 * ---------------------------------------------------------------------------*/
    00032
    00033 #include "arm_math.h"
    00034
    00078 void arm_biquad_cascade_df1_init_q15(
    00079   arm_biquad_casd_df1_inst_q15 * S,
    00080   uint8_t numStages,
    00081   q15_t * pCoeffs,
    00082   q15_t * pState,
    00083   int8_t postShift)
    00084 {
    00085   /* Assign filter stages */
    00086   S->numStages = numStages;
    00087
    00088   /* Assign postShift to be applied to the output */
    00089   S->postShift = postShift;
    00090
    00091   /* Assign coefficient pointer */
    00092   S->pCoeffs = pCoeffs;
    00093
    00094   /* Clear state buffer and size is always 4 * numStages */
    00095   memset(pState, 0, (4u * (uint32_t) numStages) * sizeof(q15_t));
    00096
    00097   /* Assign state pointer */
    00098   S->pState = pState;
    00099 }
    00100

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines