- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_fir_lattice_init_q31.c

Go to the documentation of this file.

    00001 /*-----------------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        29. November 2010
    00005 * $Revision:    V1.0.3
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_fir_lattice_init_q31.c
    00009 *
    00010 * Description:  Q31 FIR lattice filter initialization function.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3
    00013 *
    00014 * Version 1.0.3 2010/11/29
    00015 *    Re-organized the CMSIS folders and updated documentation.
    00016 *
    00017 * Version 1.0.2 2010/11/11
    00018 *    Documentation updated.
    00019 *
    00020 * Version 1.0.1 2010/10/05
    00021 *    Production release and review comments incorporated.
    00022 *
    00023 * Version 1.0.0 2010/09/20
    00024 *    Production release and review comments incorporated
    00025 *
    00026 * Version 0.0.7  2010/06/10
    00027 *    Misra-C changes done
    00028 * ---------------------------------------------------------------------------*/
    00029
    00030 #include "arm_math.h"
    00031
    00050 void arm_fir_lattice_init_q31(
    00051   arm_fir_lattice_instance_q31 * S,
    00052   uint16_t numStages,
    00053   q31_t * pCoeffs,
    00054   q31_t * pState)
    00055 {
    00056   /* Assign filter taps */
    00057   S->numStages = numStages;
    00058
    00059   /* Assign coefficient pointer */
    00060   S->pCoeffs = pCoeffs;
    00061
    00062   /* Clear state buffer and size is always numStages */
    00063   memset(pState, 0, (numStages) * sizeof(q31_t));
    00064
    00065   /* Assign state pointer */
    00066   S->pState = pState;
    00067
    00068 }
    00069

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines