- Main Page
- Modules
- Data Structures
- Files
- Examples

- File List
- Globals

# arm_biquad_cascade_df1_init_f32.c

Go to the documentation of this file.

    00001 /*-----------------------------------------------------------------------------
    00002 * Copyright (C) 2010 ARM Limited. All rights reserved.
    00003 *
    00004 * $Date:        15. July 2011
    00005 * $Revision:    V1.0.10
    00006 *
    00007 * Project:      CMSIS DSP Library
    00008 * Title:        arm_biquad_cascade_df1_init_f32.c
    00009 *
    00010 * Description:  floating-point Biquad cascade DirectFormI(DF1) filter initialization function.
    00011 *
    00012 * Target Processor: Cortex-M4/Cortex-M3/Cortex-M0
    00013 *
    00014 * Version 1.0.10 2011/7/15
    00015 *    Big Endian support added and Merged M0 and M3/M4 Source code.
    00016 *
    00017 * Version 1.0.3 2010/11/29
    00018 *    Re-organized the CMSIS folders and updated documentation.
    00019 *
    00020 * Version 1.0.2 2010/11/11
    00021 *    Documentation updated.
    00022 *
    00023 * Version 1.0.1 2010/10/05
    00024 *    Production release and review comments incorporated.
    00025 *
    00026 * Version 1.0.0 2010/09/20
    00027 *    Production release and review comments incorporated.
    00028 *
    00029 * Version 0.0.5  2010/04/26
    00030 *    incorporated review comments and updated with latest CMSIS layer
    00031 *
    00032 * Version 0.0.3  2010/03/10
    00033 *    Initial version
    00034 * ---------------------------------------------------------------------------*/
    00035
    00036 #include "arm_math.h"
    00037
    00083 void arm_biquad_cascade_df1_init_f32(
    00084   arm_biquad_casd_df1_inst_f32 * S,
    00085   uint8_t numStages,
    00086   float32_t * pCoeffs,
    00087   float32_t * pState)
    00088 {
    00089   /* Assign filter stages */
    00090   S->numStages = numStages;
    00091
    00092   /* Assign coefficient pointer */
    00093   S->pCoeffs = pCoeffs;
    00094
    00095   /* Clear state buffer and size is always 4 * numStages */
    00096   memset(pState, 0, (4u * (uint32_t) numStages) * sizeof(float32_t));
    00097
    00098   /* Assign state pointer */
    00099   S->pState = pState;
    00100 }
    00101

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Defines