LCU FPGA for 7111 with high speed connection to 7P
Revision Register reads 2234

This version is for the 7111 with high speed uplink and downlink to the Link Module through the Gigabit PHY interface. This was built starting from released version used on Ifremer. BITE is enabled. 

Note that the Link Module should be programmed with the standard release for High Speed Uplink and Downlink
