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	Date:
	11-12 Aug 2020

	Vehicle:
	I2Map

	Location:
	36.6969, -122.0470

	Major Objective:
	Overnight Transect Mission

	Dive Plan:
	Transect14_Intermediate_Ascents.cfg



Accomplishments:

· [bookmark: _GoBack]Bio-acoustics powered off, and camera data partially downloaded by R Sherlock. C Waluk will get acoustics data and R Sherlock will download the remaining videos on Aug 13, 2020 (Thursday).
· The Apollo Relay was flashing on recovery.
· Does not appear that the GPS to reset itself.
· The night dive started at 11pm as the time it should start.

Vehicle Issues:
1. The motor housing oil is cloudy so it needs to be flushed out and changed.

Note(s):
· The vehicle is rinsed. 
· The batteries will be charged on shore.
· The MVC data has been distributed and in the C:\Dorado\Data\i2map\2020.224.04 folder.
· The oil comp was fully charged on recovery.
· R Sherlock was looking at previous data from the camera and had concerns that the vehicle wasn’t programmed to reach the correct depth. The pattern was correct but his graph was stating that the vehicle only reached 500m and not 1000m. After stepping through the mission script and reviewing the MVC data off the vehicle it was concluded that the vehicle did make 100m steps down to 1000m and that the compiler that R Sherlock was using is incorrect.
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