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Description automatically generated]	AUV Post Dive Report	AUV Operations


	Date:
	13-14 Sep 2020

	Vehicle:
	I2Map

	Location:
	36.6969, -122.0470

	Major Objective:
	Overnight Transect Mission

	Dive Plan:
	Transect14_Modified.cfg



Accomplishments:

· First I2Map run on VN100 Compass.
· First dive with repaired (firmware update) SBE25p SN: 1081.
· Ran with updated QNX seabird25p driver, which supports device restart, and parameter getting at initialization time.
· Vehicle started night transects at approximately 23:18L

Vehicle Issues:
1. Camera did not stop recording at prescribed time during third 700m transect. Investigations ongoing, but appears that the camera didn’t receive or respect the stop record command. Lights powered off appropriately. No data was lost as a result of this bug, but the intent is to resolve.

Note(s):
· Vehicle was rinsed and main batteries charged while on deck.
· Acoustics sphere needs to be charged.
· Oil comp was empty on recovery.
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